{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":13,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXB-B"]
[]
[]
[]
[]
["","","","","","RXB25B5V1","RXB25B6V1","RXB25B6V19","RXB35B5V1","RXB35B6V1","RXB35B6V19","RXB50BV1B","RXB60BV1B"]
["Schalldruckpegel","Heizen","","Nom.","dB(A)","","","","","","","51","51"]
["","Kühlung","","Nom.","dB(A)","","","","","","","51","51"]
["Kältemittel","Charge","","","TCO2Eq","","","","","","","3","3"]
["","GWP","","","","","","","","","","2,087.5","2,087.5"]
["","Füllmenge","","","kg","","","","","","","1.45","1.45"]
["","Typ","","","","","","","","","","R-410A","R-410A"]
["Betriebsbereich","Kühlung","Umgebung","Max.","°C TK","","","","","","","46","46"]
["","","","Min.","°C TK","","","","","","","-10","-10"]
["","Heizen","Umgebung","Max.","°C Feuchtkugel","","","","","","","18","18"]
["","","","Min.","°C Feuchtkugel","","","","","","","-15","-15"]
["Verdichter","Type","","","","","","","","","","Hermetischer Swing","Hermetischer Swing"]
["Abmessungen","Maßeinheit","","Breite","mm","","","","","","","855","855"]
["","","","Tiefe","mm","","","","","","","328","328"]
["","","","Höhe","mm","","","","","","","753","753"]
["Gewicht","Maßeinheit","","","kg","","","","","","","44","44"]
["Spannungsversorgung","Phase","","","","","","","","","","1~","1~"]
["","Frequenz","","","Hz","","","","","","","50","50"]
["","Spannung","","","V","","","","","","","220-240","220-240"]
["Hinweise","","","","","","","","","","","(1) - Alle Geräte sind getestet und entsprechen ISO 5151 (Gerät ohne Kanal) oder ISO 13253 (Gerät mit Kanal).","(1) - Alle Geräte sind getestet und entsprechen ISO 5151 (Gerät ohne Kanal) oder ISO 13253 (Gerät mit Kanal)."]
["","","","","","","","","","","","(2) - Änderungen aller Technischen Daten durch den Hersteller ohne Ankündigung vorbehalten.","(2) - Änderungen aller Technischen Daten durch den Hersteller ohne Ankündigung vorbehalten."]
["","","","","","","","","","","","(3) - Enthält fluorierte Treibhausgase","(3) - Enthält fluorierte Treibhausgase"]
["Abmessungen","Maßeinheit","","Höhe","mm","550","550","550","550","550","550"]
["","","","Breite","mm","658","658","658","658","658","658"]
["","","","Tiefe","mm","275","275","275","275","275","275"]
["Gewicht","Maßeinheit","","","kg","27","26","26","29","28","28"]
["Verdichter","Type","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","46","46","46","48","48","48"]
["","Heizen","","Hoch","dB(A)","47","47","47","48","48","48"]
["Kältemittel","Typ","","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","Füllmenge","","","kg","0.74","0.74","0.74","1.00","1.00","1.00"]
["","Füllmenge","","","tCO2Eq","1.5","1.5","1.5","2.1","2.1","2.1"]
["","GWP","","","","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","m","15","15","15","15","15","15"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","IG - AG","Max.","m","12","12","12","12","12","12"]
["Standardzubehör","Installation manual","","","","1","1","1","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1"]
["Stromversorgung","Phase","","","","1~","1~","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C TK","","-10","-10","","-10","-10"]
["","","","Max.","°C TK","","46","46","","46","46"]
["","Heizen","Umgebung","Min.","°C Feuchtkugel","","-15","-15","","-15","-15"]
["","","","Max.","°C Feuchtkugel","","18","18","","18","18"]