{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":58,"n_cols":11,"rows_kept":58,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXG-K"]
[]
[]
[]
[]
["","","","","","RXG25K3V1B","RXG25K2V1B","RXG35K3V1B","RXG35K2V1B","RXG50K3V1B","RXG50K2V1B"]
["Schalldruckpegel","Heizen","","Hoch","dB(A)","47","","48","","48"]
["","Kühlung","","Hoch","dB(A)","46","","48","","48"]
["Kältemittel","Charge","","","TCO2Eq","2.2","","2.2","","3.3"]
["","GWP","","","","2,087.5","","2,087.5","","2,087.5"]
["","Charge","","","kg","1.05","","1.05","","1.6"]
["","Typ","","","","R-410A","","R-410A","","R-410A"]
["Ventilatormotor","Drehzahl","Kühlung","Sehr niedrig","U/min","780","","780","","670"]
["","","Heizen","Sehr niedrig","U/min","740","","740","","670"]
["Rohrleitungsanschlüsse","Niveauunterschied","IG - AG","Max.","m","15","","15","","20"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)","","0,02 (für Rohrleitungslängen über 10 m)","","0,02 (für Rohrleitungslängen über 10 m)"]
["Verdichter","Typ","","","","Vollhermetischer Schwingverdichter","","Vollhermetischer Schwingverdichter","","Vollhermetischer Schwingverdichter"]
["Abmessungen","Maßeinheit","","Breite","mm","765","","765","","825"]
["","","","Tiefe","mm","285","","285","","300"]
["","","","Höhe","mm","550","","550","","735"]
["Gewicht","Maßeinheit","","","kg","34","","34","","48"]
["Ventilator","Luftstromvolumen","Heizen","Sehr niedrig","cfm","904","","904","","1,522"]
["","","Kühlung","Sehr niedrig","cfm","1,063","","1,063","","1,727"]
["Power supply","Phase","","","","1~","","1~","","1~"]
["","Frequenz","","","Hz","50","","50","","50"]
["","Spannung","","","V","220-240","","220-240","","220-240"]
["Hinweise","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["","","","","","(4) - Betriebsbereich in Kombination mit Nexura, FVXG-K: min. 10°C TK bis max. 46°C TK","(4) - Betriebsbereich in Kombination mit Nexura, FVXG-K: min. 10°C TK bis max. 46°C TK","(4) - Betriebsbereich in Kombination mit Nexura, FVXG-K: min. 10°C TK bis max. 46°C TK","(4) - Betriebsbereich in Kombination mit Nexura, FVXG-K: min. 10°C TK bis max. 46°C TK","(4) - Betriebsbereich in Kombination mit Nexura, FVXG-K: min. 10°C TK bis max. 46°C TK","(4) - Betriebsbereich in Kombination mit Nexura, FVXG-K: min. 10°C TK bis max. 46°C TK"]
["","","","","","(5) - Enthält fluorierte Treibhausgase","","(5) - Enthält fluorierte Treibhausgase","","(5) - Enthält fluorierte Treibhausgase"]
["Ventilator","Luftstromvolumen","Kühlung","Sehr niedrig","m³/min","","30.1","","30.1","","48.9"]
["","","Heizen","Sehr niedrig","m³/min","","25.6","","25.6","","43.1"]
["","","","Sehr niedrig","cfm","","1063","","1063","","1727"]
["","","Heizen","Sehr niedrig","cfm","","904","","904","","1522"]
["Abmessungen","Maßeinheit","","Höhe","mm","","550","","550","","735"]
["","","","Breite","mm","","765","","765","","825"]
["","","","Tiefe","mm","","285","","285","","300"]
["Gewicht","Maßeinheit","","","kg","","34","","34","","48"]
["Ventilatormotor","Drehzahl","Kühlung","Sehr niedrig","U/min","","780","","780","","670"]
["","","Heizen","Sehr niedrig","U/min","","740","","740","","670"]
["Verdichter","Typ","","","","","Vollhermetischer Swing-Verdichter","","Vollhermetischer Swing-Verdichter","","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C TK","","-10","","-10","","-10"]
["","","","Max.","°C TK","","46","","46","","46"]
["","Heizen","Umgebung","Min.","°C FK","","-15","","-15","","-15"]
["","","","Max.","°C FK","","20","","20","","20"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","","46","","48","","48"]
["","Heizen","","Hoch","dB(A)","","47","","48","","48"]
["Kältemittel","Typ","","","","","R-410A","","R-410A","","R-410A"]
["","Füllmenge","","","kg","","1.05","","1.05","","1.6"]
["","Füllmenge","","","tCO2Eq","","2.2","","2.2","","3.3"]
["","GWP","","","","","2087.5","","2087.5","","2087.5"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","m","","20","","20","","30"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","","0,02 (für Rohrleitungslängen über 10 m)","","0,02 (für Rohrleitungslängen über 10 m)","","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","IG - AG","Max.","m","","15","","15","","20"]
["Stromversorgung","Phase","","","","","1~","","1~","","1~"]
["","Frequenz","","","Hz","","50","","50","","50"]
["Spannungsversorgung","Spannung","","","V","","220-240","","220-240","","220-240"]