{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":16,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXJ-M"]
[]
[]
[]
[]
["","","","","","RXJ20M2V1B","RXJ20M3V1B","RXJ20M5V1B","RXJ25M2V1B","RXJ25M3V1B","RXJ25M5V1B","RXJ35M2V1B","RXJ35M3V1B","RXJ35M5V1B","RXJ50MV1B","RXJ50M2V1B"]
["Ventilator","Luftstromvolumen","Kühlung","Sehr niedrig","m³/min","29.3","","","29.3","","","29.3","","","38.5"]
["","","Heizen","Sehr niedrig","m³/min","25.6","","","25.6","","","25.6","","","34.3"]
["","","","Sehr niedrig","cfm","1035","","","1035","","","1035","","","1359"]
["","","Heizen","Sehr niedrig","cfm","904","","","904","","","904","","","1211"]
["Abmessungen","Maßeinheit","","Höhe","mm","550","550","550","550","550","550","550","550","550","735","735"]
["","","","Breite","mm","765","765","765","765","765","765","765","765","765","825","825"]
["","","","Tiefe","mm","285","285","285","285","285","285","285","285","285","300","300"]
["Gewicht","Maßeinheit","","","kg","34","32","32","34","32","32","34","32","32","44","44"]
["Ventilatormotor","Drehzahl","Kühlung","Sehr niedrig","U/min","760","","","760","","","760","","","620"]
["","","Heizen","Sehr niedrig","U/min","740","","","740","","","740","","","620"]
["Verdichter","Typ","","","","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C TK","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10"]
["","","","Max.","°C TK","46","46","46","46","46","46","46","46","46","46","46"]
["","Heizen","Umgebung","Min.","°C FK","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15"]
["","","","Max.","°C FK","18","18","18","18","18","18","18","18","18","18","20"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","46","","","46","","","48","","","48","48"]
["","","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dBA","","46","46","","46","46","","49","49"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dBA","","","","","","","","","","","45"]
["","Heizen","","Hoch","dBA","47","","","47","","","48","","","48","48"]
["","","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dBA","","47","47","","47","47","","49","49"]
["","","","Niedrig","dBA","","","","","","","","","","","45"]
["Kältemittel","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Füllmenge","","","kg","0.72","0.76","0.76","0.72","0.76","0.76","0.72","0.76","0.76","1.30","1.3"]
["","Füllmenge","","","tCO2Eq","0.5","0.52","0.52","0.5","0.52","0.52","0.5","0.52","0.52","0.9","0.88"]
["","GWP","","","","675","675.0","675.0","675","675.0","675.0","675","675.0","675.0","675","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","M","20","20","20","20","20","20","20","20","20","30","30"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","IG - AG","Max.","M","15","15.0","15.0","15","15.0","15.0","15","15.0","15.0","20"]
["Standardzubehör","Installation manual","","","","1","1","","1","1","","1","1","","1"]
["","Drain plug","","","","1","1","","1","1","","1","1","","1"]
["Stromversorgung","Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50","50","50","50","50","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Hinweise","","","","","(1) - 220 V","","","(1) - 220 V","","","(1) - 220 V","","","(1) - 220 V"]
["","","","","","(2) - 230 V","","","(2) - 230 V","","","(2) - 230 V","","","(2) - 230 V"]
["","","","","","(3) - 240 V","","","(3) - 240 V","","","(3) - 240 V","","","(3) - 240 V"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Standardzubehör","Refrigerant charge label","","","","","1","","","1","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","","1","","","1","","","1"]
["","General safety precautions","","","","","1","","","1","","","1"]