{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":10,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXL-K"]
[]
[]
[]
[]
["","","","","","RXL20K3V1B","RXL25K3V1B","RXL35K2V1B","RXL42K2V1B","RXL50K2V1B"]
["Ventilator","Luftstromvolumen","Kühlung","Sehr niedrig","m³/min","","","30.1","30.6","48.9"]
["","","Heizen","Sehr niedrig","m³/min","","","25.6","27.2","43.1"]
["","","","Sehr niedrig","cfm","","","1063","1080","1727"]
["","","Heizen","Sehr niedrig","cfm","","","904","960","1522"]
["Abmessungen","Maßeinheit","","Höhe","mm","550","550","550","550","735"]
["","","","Breite","mm","765","765","765","765","825"]
["","","","Tiefe","mm","285","285","285","285","300"]
["Gewicht","Maßeinheit","","","kg","34","34","34","39","47"]
["Ventilatormotor","Drehzahl","Kühlung","Sehr niedrig","U/min","780","780","780","790","670"]
["","","Heizen","Sehr niedrig","U/min","740","740","740","780","670"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C TK","-10","-10","-10","-10","-10"]
["","","","Max.","°C TK","46","46","46","46","46"]
["","Heizen","Umgebung","Min.","°C Feuchtkugel","-25","-25","-25","-25","-25"]
["","","","Max.","°C Feuchtkugel","18","18","18","18","18"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","46","46","48","48","48"]
["","Heizen","","Hoch","dBA","47","47","48","48","48"]
["Kältemittel","Typ","","","","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","Füllmenge","","","kg","1.0","1.05","1.2","1.3","1.7"]
["","Füllmenge","","","tCO2Eq","2.1","2.2","2.5","2.7","3.5"]
["","GWP","","","","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","M","20","20","20","20","30"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","IG - AG","Max.","M","15","15","15","15","20"]
["Standardzubehör","Installation manual","","","","1","1","1","1","1"]
["","Drain plug","","","","1"]
["Stromversorgung","Phase","","","","1~","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240","220-230-240","220-230-240","220-230-240"]
["Hinweise","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]