{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXLG-M"]
[]
[]
[]
[]
["","","","","","RXLG25M2V1B","RXLG35M2V1B"]
["Ventilator","Luftstromvolumen","Kühlung","Sehr niedrig","m³/min","30.6","30.6"]
["","","Heizen","Sehr niedrig","m³/min","27.2","27.2"]
["","","","Sehr niedrig","cfm","1080","1080"]
["","","Heizen","Sehr niedrig","cfm","960","960"]
["Abmessungen","Maßeinheit","","Höhe","mm","550","550"]
["","","","Breite","mm","858","858"]
["","","","Tiefe","mm","330","330"]
["Gewicht","Maßeinheit","","","kg","40","40"]
["Verdichter","Typ","","","","","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°CTK","-10","-10"]
["","","","Max.","°CTK","46","46"]
["","Heizen","Umgebung","Min.","°C FK","-25","-25"]
["","","","Max.","°C FK","18","18"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","48","48"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dBA","44","44"]
["","Heizen","","Hoch","dBA","49","49"]
["","","","Niedrig","dBA","45","45"]
["Kältemittel","Typ","","","","R-410A","R-410A"]
["","Füllmenge","","","kg","1","1"]
["","Füllmenge","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","M","20","20"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","IG - IG","Max.","M","15","15"]
["Standardzubehör","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["Stromversorgung","Phase","","","","1~","1~"]
["","Frequenz","","","Hz","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter"]