{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":13,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-M"]
[]
[]
[]
[]
["","","","","","RXM20M2V1B","RXM25M2V1B","RXM35M2V1B","RXM42M2V1B","RXM50M2V1B","RXM50MV1B","RXM60M2V1B","RXM71M2V1B"]
["Abmessungen","Maßeinheit","","Höhe","mm","550","550","550","735","735","735","735","734"]
["","","","Breite","mm","765","765","765","825","825","825","825","870"]
["","","","Tiefe","mm","285","285","285","300","300","300","300","320"]
["Gewicht","Maßeinheit","","","kg","32","32","32","47","47","44","44","56"]
["Compressor","Typ","","","","","Vollhermetischer Swing-Verdichter","","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C Trockenkugel","-10","-10","-10","-10 (1)","-10 (1)","-10","-10","-10"]
["","","","Max.","°C Trockenkugel","46","46","46","46 (1)","46 (1)","46","46","46"]
["","Heizen","Umgebung","Min.","°C Feuchtkugel","-15","-15","-15","-15","-15","-15","-15","-15"]
["","","","Max.","°C Feuchtkugel","18","18","18","18","18","18","18","18"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","46","46","49","","","48","48"]
["","","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dBA","","","","48","48","","","47"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dBA","","","","","","44","44"]
["","Heizen","","Hoch","dBA","47","47","49","","","49","49"]
["","","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dBA","","","","48","49","","","48"]
["","","","Niedrig","dBA","","","","","","45","45"]
["Kältemittel","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Füllmenge","","","kg","0.76","0.76","0.76","1.30","1.40","1.4","1.45","1.15"]
["","Füllmenge","","","tCO2Eq","0.5","0.5","0.5","0.88","0.95","0.9","1.0","0.78"]
["","GWP","","","","675","675","675","675","675","675","675","675.0"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","M","30","30","30","30","30","30","30","30.0"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","IG - AG","Max.","M","20","20","20","20","20","20","20","20.0"]
["Standardzubehör","Installation manual","","","","1","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1","1"]
["","Drain plug (only heat pump models)","","","","1","1","1","","","1","1"]
["Stromversorgung","Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50","50","50","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Standardzubehör","Drain plug","","","","","","","1","1","","","1"]
["Hinweise","","","","","","","","(1) - Siehe separate Zeichnung für den Betriebsbereich","(1) - Siehe separate Zeichnung für den Betriebsbereich","","","(1) - Siehe separate Zeichnung für den Betriebsbereich"]
["Standardzubehör","Drain cap","","","","","","","","","","","3"]