{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":9,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-N"]
[]
[]
[]
[]
["","","","","","RXM42N2V1B","RXM50N2V1B","RXM60N2V1B","RXM71N2V1B"]
["Abmessungen","Maßeinheit","","Höhe","mm","734","734","734","734"]
["","","","Breite","mm","870","870","870","870"]
["","","","Tiefe","mm","373","373","373","320"]
["Gewicht","Maßeinheit","","","kg","50","50","50","56"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°CTK","-10","-10","-10","-10"]
["","","","Max.","°CTK","46","46","46","46"]
["","Heizen","Umgebung","Min.","°C FK","-15","-15","-15","-15"]
["","","","Max.","°C FK","18","18","18","18"]
["Schalldruckpegel","Kühlung","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dB(A)","48.0","48.0","48.0","47"]
["","Heizen","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dB(A)","48.0","49.0","49.0","48"]
["Kältemittel","Typ","","","","R-32","R-32","R-32","R-32"]
["","Füllmenge","","","kg","1.10","1.15","1.15","1.15"]
["","Füllmenge","","","tCO2Eq","0.75","0.78","0.78","0.78"]
["","GWP","","","","675","675","675","675.0"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","m","30","30","30","30.0"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","IG - AG","Max.","m","20","20","20","20.0"]
["Standardzubehör","Installation manual","","","","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1"]
["","Drain cap","","","","3","3","3","3"]
["","Drain plug","","","","1","1","1","1"]
["Stromversorgung","Phase","","","","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240","220-240","220-240"]
["Verdichter","Typ","","","","","Vollhermetischer Swing-Verdichter"]