{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":14,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXP-L"]
[]
[]
[]
[]
["","","","","","RXP20L2V1B","RXP20L5V1B","RXP25L2V1B","RXP25L5V1B","RXP35L2V1B","RXP35L5V1B","RXP50L2V1B","RXP60L2V1B","RXP71L2V1B"]
["Abmessungen","Maßeinheit","","Höhe","mm","550","550","550","550","550","550","734","734","734"]
["","","","Breite","mm","658","658","658","658","658","658","870","870","870"]
["","","","Tiefe","mm","275","275","275","275","275","275","373","373","373"]
["Gewicht","Maßeinheit","","","kg","28","26","28","26","28","28","46.0","50.0","50.0"]
["Compressor","Typ","","","","","","","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C TK","-10","","-10","","-10","","-10","-10","-10"]
["","","","Max.","°C TK","46","","46","","46","","46","46","46"]
["","Heizen","Umgebung","Min.","°C Feuchtkugel","-15","","-15","","-15","","-15","-15","-15"]
["","","","Max.","°C Feuchtkugel","18","","18","","18","","18","18","18"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","46","46","46","46","48","48"]
["","","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dBA","","","","","","","47","49","52"]
["","Heizen","","Hoch","dBA","47","47","47","47","48","48"]
["","","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dBA","","","","","","","49","49","52"]
["Kältemittel","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Füllmenge","","","kg","0.70","0.65","0.70","0.65","0.70","0.70","0.90","1.15","1.15"]
["","Füllmenge","","","tCO2Eq","0.48","0.44","0.48","0.44","0.48","0.48","0.61","0.78","0.78"]
["","GWP","","","","675.0","675.0","675.0","675.0","675.0","675.0","675","675","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","M","15","15","15","15","15","15","30","30","30"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","IG - AG","Max.","M","12","12","12","12","12","12","20","20","20"]
["Standardzubehör","Installation manual","","","","1","1","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1","1","1"]
["","Drain cap","","","","","","","","","","3","3","3"]
["","Drain plug","","","","1","1","1","1","1","1","1","1","1"]
["Stromversorgung","Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50","50","50","50","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Standardzubehör","General safety precautions","","","","1","1","1","1","1","1"]