{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F"]
[]
[]
[]
[]
["","","","","","RXS60F4V1B","RXS60F2V1B","RXS60F3V1B","RXS71FAV1B9","RXS71FV1B","RXS71FAV1B"]
["Schalldruckpegel","Heizen","","Hoch","dBA","49","","","52"]
["","","","Niedrig","dBA","46","","","49"]
["","Kühlung","","Niedrig","dBA","46","","","49"]
["","","","Hoch","dBA","49","","","52"]
["Standardzubehör","Kondensatmuffe","","","","1","","","1"]
["","Installationsanleitung","","","","1","","","1"]
["Kältemittel","Charge","","","TCO2Eq","3.1","","","4.8"]
["","GWP","","","","2,087.5","","","2,087.5"]
["","Füllmenge","","","kg","1.5","","","2.3"]
["","Typ","","","","R-410A","","","R-410A"]
["Rohrleitungsanschlüsse","Niveauunterschied","IG - AG","Max.","M","20","","","20"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)","","","0,02 (für Rohrleitungslängen über 10 m)"]
["Verdichter","Type","","","","Vollhermetischer Schwingverdichter","","","Vollhermetischer Schwingverdichter"]
["Abmessungen","Maßeinheit","","Breite","mm","825","","","900"]
["","","","Tiefe","mm","300","","","320"]
["","","","Höhe","mm","735","","","770"]
["Gewicht","Maßeinheit","","","kg","48","","","71"]
["Power supply","Phase","","","","1~","","","1~"]
["","Frequenz","","","Hz","50","","","50"]
["","Spannung","","","V","220-240","","","220-240"]
["Hinweise","","","","","(1) - SL: Die flüsterleise Ventilatorstufe der Luftmengeneinstellung.","(1) - 220 V","","(1) - SL: Die flüsterleise Ventilatorstufe der Luftmengeneinstellung.","(1) - 220 V"]
["","","","","","(2) - Enthält fluorierte Treibhausgase","(2) - 230 V","","(2) - Enthält fluorierte Treibhausgase","(2) - 230 V"]
["Abmessungen","Maßeinheit","","Höhe","mm","","735","735","","770","770"]
["","","","Breite","mm","","825","825","","900","900"]
["","","","Tiefe","mm","","300","300","","320","320"]
["Gewicht","Maßeinheit","","","kg","","48","48","","71","71"]
["Verdichter","Type","","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C TK","","-10","-10","","-10","-10"]
["","","","Max.","°C TK","","46","46","","46","46"]
["","Heizen","Umgebung","Min.","°C Feuchtkugel","","-15","-15","","-15","-15"]
["","","","Max.","°C Feuchtkugel","","18","20","","18","20"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","","49","49","","52","52"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dBA","","46","46","","49","49"]
["","Heizen","","Hoch","dBA","","49","49","","52","52"]
["","","","Niedrig","dBA","","46","46","","49","49"]
["Kältemittel","Typ","","","","","R-410A","R-410A","","R-410A","R-410A"]
["","Füllmenge","","","kg","","1.5","1.5","","2.3","2.3"]
["","Füllmenge","","","tCO2Eq","","3.1","3.1","","4.8","4.8"]
["","GWP","","","","","2087.5","2087.5","","2087.5","2087.5"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","M","","30","30","","30","30"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","IG - AG","Max.","M","","20","20","","20","20"]
["Standardzubehör","Installation manual","","","","","Installation manual","1","","Installation manual","1"]
["","Drain plug","","","","","Drain plug","","","Drain plug"]
["Stromversorgung","Phase","","","","","1~","1~","","1~","1~"]
["","Frequenz","","","Hz","","50","50","","50","50"]
["Spannungsversorgung","Spannung","","","V","","220-240","220-240","","220-240","220-240"]
["Hinweise","","","","","","(3) - 240 V","","","(3) - 240 V"]
["Standardzubehör","Drain socket","","","","","","1","","","1"]
["Sound power level","Kühlung","","","dBA","","","","65"]