{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":6,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F8"]
[]
[]
[]
[]
["","","","","","RXS71FAV1B8"]
["Ventilator","Luftstromvolumen","Kühlung","Sehr niedrig","m³/min","46.0"]
["","","Heizen","Sehr niedrig","m³/min","46.0"]
["","","","Sehr niedrig","cfm","1624"]
["","","Heizen","Sehr niedrig","cfm","1624"]
["Abmessungen","Maßeinheit","","Höhe","mm","770"]
["","","","Breite","mm","900"]
["","","","Tiefe","mm","320"]
["Gewicht","Maßeinheit","","","kg","71"]
["Ventilatormotor","Drehzahl","Kühlung","Sehr niedrig","U/min","730"]
["","","Heizen","Sehr niedrig","U/min","730"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°CTK","-10"]
["","","","Max.","°CTK","46"]
["","Heizen","Umgebung","Min.","°C FK","-15"]
["","","","Max.","°C FK","18"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","52"]
["","Heizen","","Hoch","dBA","52"]
["Kältemittel","Typ","","","","R-410A"]
["","Füllmenge","","","kg","2.3"]
["","Füllmenge","","","tCO2Eq","4.8"]
["","GWP","","","","2087.5"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","M","30"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","IG - AG","Max.","M","20"]
["Standardzubehör","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain socket assy","","","","1"]
["Stromversorgung","Phase","","","","1~"]
["","Frequenz","","","Hz","50"]
["Spannungsversorgung","Spannung","","","V","220-240"]
["Hinweise","","","","","(1) - 220 V"]
["","","","","","(2) - 230 V"]
["","","","","","(3) - 240 V"]