{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":73,"n_cols":11,"rows_kept":73,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L"]
[]
[]
[]
[]
["","","","","","RXS20L2V1B","RXS25L2V1B","RXS35L2V1B","RXS42L2V1B","RXS50L2V1B","RXS60L2V1B"]
["Schalldruckpegel","Heizen","","Hoch","dBA","47","47","48","48"]
["","Kühlung","","Hoch","dBA","46","46","48","48"]
["Standardzubehör","Kondensatkappe","","","","1","1","","1"]
["","Installationsanleitung","","","","1","1","1","1"]
["","Etikett für Kältemittelfüllmenge","","","","1","1","1"]
["","Mehrsprachige Etiketten über fluorierte Treibhausgase","","","","1","1","Mehrsprachige Etiketten über fluorierte Treibhausgase"]
["Kältemittel","Charge","","","TCO2-Äquivalent","2.1","2.1","2.5","2.7"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Füllmenge","","","kg","1.0","1.0","1.20","1.3"]
["","Typ","","","","R-410A","R-410A","R-410A","R-410A"]
["Ventilatormotor","Drehzahl","Kühlung","Sehr niedrig","U/min","780","780","780","790"]
["","","Heizen","Sehr niedrig","U/min","740","740","740","780"]
["Betriebsbereich","Kühlung","Umgebung","Max.","°C Trockenkugel","46","46","46","46"]
["","","","Min.","°C Trockenkugel","-10","-10","-10","-10"]
["","Heizen","Umgebung","Max.","°C FK","18","18","18","18"]
["","","","Min.","°C FK","-15","-15","-15","-15"]
["Rohrleitungsanschlüsse","Niveauunterschied","IG - AG","Max.","M","","","15"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","","","0,020 (für Rohrleitungslängen über 10 m)"]
["Abmessungen","Maßeinheit","","Breite","mm","765","765","765","765"]
["","","","Tiefe","mm","285","285","285","285"]
["","","","Höhe","mm","550","550","550","550"]
["Verdichter","Typ","","","","Vollhermetischer Schwingverdichter","Vollhermetischer Schwingverdichter","Vollhermetischer Schwingverdichter","Vollhermetischer Schwingverdichter"]
["Gewicht","Maßeinheit","","","kg","34","34","34","39"]
["Ventilator","Luftstromvolumen","Heizen","Sehr niedrig","cfm","904","904","904","960"]
["","","","Sehr niedrig","m³/min","25.6","25.6","25.6","27.2"]
["","","Kühlung","Sehr niedrig","m³/min","30.1","30.1","30.1","30.6"]
["","","","Sehr niedrig","cfm","1,063","1,063","1,063","1,080"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50","50"]
["","Spannung","","","V","220-240","220-240","220-240","220-240"]
["Hinweise","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["","","","","","(4) - Enthält fluorierte Treibhausgase","(4) - Enthält fluorierte Treibhausgase","(4) - Enthält fluorierte Treibhausgase","(4) - Enthält fluorierte Treibhausgase"]
["Standardzubehör","Ablassstopfen","","","","","","1"]
["Ventilator","Luftstromvolumen","Kühlung","Sehr niedrig","m³/min","","","","","48.9","45.0"]
["","","Heizen","Sehr niedrig","m³/min","","","","","43.1","46.3"]
["","","","Sehr niedrig","cfm","","","","","1727","1589"]
["","","Heizen","Sehr niedrig","cfm","","","","","1522","1635"]
["Abmessungen","Maßeinheit","","Höhe","mm","","","","","735","735"]
["","","","Breite","mm","","","","","825","825"]
["","","","Tiefe","mm","","","","","300","300"]
["Gewicht","Maßeinheit","","","kg","","","","","47","48"]
["Ventilatormotor","Drehzahl","Kühlung","Sehr niedrig","U/min","","","","","670"]
["","","Heizen","Sehr niedrig","U/min","","","","","670"]
["Verdichter","Typ","","","","","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C Trockenkugel","","","","","-10","-10"]
["","","","Max.","°C Trockenkugel","","","","","46","46"]
["","Heizen","Umgebung","Min.","°C FK","","","","","-15","-15"]
["","","","Max.","°C FK","","","","","18","18"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","","","","","48","49"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dBA","","","","","44","46"]
["","Heizen","","Hoch","dBA","","","","","48","49"]
["","","","Niedrig","dBA","","","","","45","46"]
["Kältemittel","Typ","","","","","","","","R-410A","R-410A"]
["","Füllmenge","","","kg","","","","","1.7","1.5"]
["","Füllmenge","","","tCO2Eq","","","","","3.5","3.1"]
["","GWP","","","","","","","","2087.5","2087.5"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","M","","","","","30","30"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","","","","","0,020 (für Rohrleitungslängen über 10 m)","0,020 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","IG - AG","Max.","M","","","","","20.0","20"]
["Standardzubehör","Installation manual","","","","","","","","1","1"]
["","Drain plug","","","","","","","","1","1"]
["Stromversorgung","Phase","","","","","","","","1~","1~"]
["","Frequenz","","","Hz","","","","","50","50"]
["Spannungsversorgung","Spannung","","","V","","","","","220-230-240","220-230-240"]
["Hinweise","","","","","","","","","","(1) - 230 V"]