{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":6,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTA-B"]
[]
[]
[]
[]
["","","","","","RXTA30B2V1B"]
["Abmessungen","Maßeinheit","","Höhe","mm","551"]
["","","","Breite","mm","763"]
["","","","Tiefe","mm","312"]
["Gewicht","Maßeinheit","","","kg","38"]
["Ventilatormotor","Drehzahl","Kühlung","Sehr niedrig","U/min","450"]
["","","Heizen","Sehr niedrig","U/min","360"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C TK","-10"]
["","","","Max.","°C TK","46"]
["","Heizen","Umgebung","Min.","°C FK","-25"]
["","","","Max.","°C FK","18"]
["Schalldruckpegel","Kühlung","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dB(A)","48"]
["","Heizen","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dB(A)","49"]
["Kältemittel","Typ","","","","R-32"]
["","Füllmenge","","","kg","1.1"]
["","Füllmenge","","","tCO2Eq","0.74"]
["","GWP","","","","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","m","20"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","IG - AG","Max.","m","15"]
["Standardzubehör","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["Stromversorgung","Phase","","","","1~"]
["","Frequenz","","","Hz","50"]
["Spannungsversorgung","Spannung","","","V","220-240"]