{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTP-N9"]
[]
[]
[]
[]
["","","","","","RXTP25N2V1B9","RXTP35N2V1B9"]
["Schalldruckpegel","Heizen","","Nom.","dBA","49","49"]
["","Kühlung","","Nom.","dBA","48","48"]
["Standardzubehör","Installationsanleitung","","","","1","1"]
["","Etikett für Kältemittelfüllmenge","","","","1","1"]
["","Mehrsprachige Etiketten über fluorierte Treibhausgase","","","","1","1"]
["Kältemittel","Charge","","","TCO2Eq","0.75","0.75"]
["","GWP","","","","675","675"]
["","Charge","","","kg","1.1","1.1"]
["","Typ","","","","R-32","R-32"]
["Ventilatormotor","Drehzahl","Kühlung","Sehr niedrig","U/min","450","450"]
["","","Heizen","Sehr niedrig","U/min","360","360"]
["Betriebsbereich","Kühlung","Umgebung","Max.","°C TK","46","46"]
["","","","Min.","°C TK","-10","-10"]
["","Heizen","Umgebung","Max.","°C Feuchtkugel","18","18"]
["","","","Min.","°C Feuchtkugel","-25","-25"]
["Rohrleitungsanschlüsse","Niveauunterschied","IG - AG","Max.","M","15","15"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)"]
["Verdichter","Typ","","","","Vollhermetischer Schwingverdichter","Vollhermetischer Schwingverdichter"]
["Abmessungen","Gerät","","Breite","mm","763","763"]
["","","","Tiefe","mm","312","312"]
["","","","Höhe","mm","551","551"]
["Gewicht","Maßeinheit","","","kg","38","38"]
["Power supply","Phase","","","","1~","1~"]
["","Frequenz","","","Hz","50","50"]
["","Spannung","","","V","220-240","220-240"]
["Hinweise","","","","","(1) - Enthält fluorierte Treibhausgase","(1) - Enthält fluorierte Treibhausgase"]
["","","","","","(2) - Siehe separate Zeichnung für den Betriebsbereich","(2) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","(3) - Siehe separate Zeichnung für die elektrischen Daten","(3) - Siehe separate Zeichnung für die elektrischen Daten"]