{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":11,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXZ-N"]
[]
[]
[]
[]
["","","","","","RXZ25NV1B","RXZ25NV1B9","RXZ35NV1B","RXZ35NV1B9","RXZ50NV1B","RXZ50NV1B9"]
["Schalldruckpegel","Heizen","","Hoch","dB(A)","","","48","48","50","50"]
["","Kühlung","","Hoch","dB(A)","","","48","48","49","49"]
["Standardzubehör","Bedienungsanleitung","","","","","","1","1","1","1"]
["","Installationsanleitung","","","","","","1","1","1","1"]
["Kältemittel","GWP","","","","","","675","675","675","675"]
["","Charge","","","kg","","","1.34","1.34","1.34","1.34"]
["","Typ","","","","","","R-32","R-32","R-32","R-32"]
["Betriebsbereich","Kühlung","Umgebung","Max.","°C Trockenkugel","","","43","43","43","43"]
["","","","Min.","°C Trockenkugel","","","-10","-10","-10","-10"]
["","Heizen","Umgebung","Max.","°C Feuchtkugel","","","18","18","18","18"]
["","","","Min.","°C Feuchtkugel","","","-20","-20","-20","-20"]
["Rohrleitungsanschlüsse","Niveauunterschied","IG - AG","Max.","m","","","8","8","8","8"]
["Abmessungen","Maßeinheit","","Breite","mm","","","795","795","795","795"]
["","","","Tiefe","mm","","","300","300","300","300"]
["","","","Höhe","mm","","","693","693","693","693"]
["Verdichter","Typ","","","","","","Vollhermetischer Schwingverdichter","Vollhermetischer Schwingverdichter","Vollhermetischer Schwingverdichter","Vollhermetischer Schwingverdichter"]
["Gewicht","Maßeinheit","","","kg","","","50","50","50","50"]
["Power supply","Phase","","","","","","1~","1~","1~","1~"]
["","Frequenz","","","Hz","","","50","50","50","50"]
["","Spannung","","","V","","","220-240","220-240","220-240","220-240"]
["Hinweise","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["","","","","","","","(4) - Enthält fluorierte Treibhausgase","(4) - Enthält fluorierte Treibhausgase","(4) - Enthält fluorierte Treibhausgase","(4) - Enthält fluorierte Treibhausgase"]
["Abmessungen","Maßeinheit","","Höhe","mm","693","693"]
["","","","Breite","mm","795","795"]
["","","","Tiefe","mm","300","300"]
["Gewicht","Maßeinheit","","","kg","50","50"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C Trockenkugel","-10","-10"]
["","","","Max.","°C Trockenkugel","43","43"]
["","Heizen","Umgebung","Min.","°C Feuchtkugel","-20","-20"]
["","","","Max.","°C Feuchtkugel","18","18"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","46","46"]
["","Heizen","","Hoch","dB(A)","46","46"]
["Kältemittel","Typ","","","","R-32","R-32"]
["","Füllmenge","","","kg","1.34","1.34"]
["","Füllmenge","","","tCO2Eq","0.9","0.9"]
["","GWP","","","","675","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","m","10","10"]
["","Niveauunterschied","IG - AG","Max.","m","8","8"]
["Standardzubehör","Installation manual","","","","1","1"]
["","Operation manual","","","","1","1"]
["Stromversorgung","Phase","","","","1~","1~"]
["","Frequenz","","","Hz","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240"]