{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-B"]
[]
[]
[]
[]
["","","","","","RZAG35B5V1B","RZAG50B5V1B","RZAG60B5V1B"]
["Abmessungen","Maßeinheit","","Höhe","mm","734","734","734"]
["","","","Breite","mm","870","870","870"]
["","","","Tiefe","mm","373","373","373"]
["Gewicht","Maßeinheit","","","kg","52","52","52"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C TK","-20","-20","-20"]
["","","","Max.","°C TK","52","52","52"]
["","Heizen","Umgebung","Min.","°C FK","-21","-21","-21"]
["","","","Max.","°C FK","18","18","18"]
["Schallleistungspegel","Kühlung","","","dB(A)","62","63","64"]
["","Heizen","","","dB(A)","62","63","64"]
["Schalldruckpegel","Kühlung","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dB(A)","48","49","50"]
["","Heizen","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dB(A)","48","49","50"]
["Kältemittel","Typ","","","","R-32","R-32","R-32"]
["","Füllmenge","","","kg","1.55","1.55","1.55"]
["","GWP","","","","675","675","675"]
["","Füllmenge","","","tCO2Eq","1.05","1.05","1.05"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35","6.35","6.35"]
["","Gas","","AD","mm","9.52","12.7","12.7"]
["","Leitungslänge","Max.","AG – IG","m","50","50","50"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 30 m)","0,02 (für Rohrleitungslängen über 30 m)","0,02 (für Rohrleitungslängen über 30 m)"]
["","Niveauunterschied","IG - AG","Max.","m","30","30","30"]
["Standardzubehör","RZAG35B5V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","General safety precautions","General safety precautions","General safety precautions"]
["","LOT10 Energy Label","","","","LOT10 Energy Label","LOT10 Energy Label","LOT10 Energy Label"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Stromversorgung","Phase","","","","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240","220-240"]
["Hinweise","","","","","(1) - Siehe separate Zeichnung für den Betriebsbereich","(1) - Siehe separate Zeichnung für den Betriebsbereich","(1) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","(2) - Siehe separate Zeichnung für die elektrischen Daten","(2) - Siehe separate Zeichnung für die elektrischen Daten","(2) - Siehe separate Zeichnung für die elektrischen Daten"]
["","","","","","(3) - Enthält fluorierte Treibhausgase","(3) - Enthält fluorierte Treibhausgase","(3) - Enthält fluorierte Treibhausgase"]
["Standardzubehör","RZAG50B5V1B","","","","","1"]
["","RZAG60B5V1B","","","","","","1"]