{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":74,"n_cols":9,"rows_kept":74,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-MV1"]
[]
[]
[]
[]
["","","","","","RZAG71M7V1B","RZAG100M7V1B","RZAG125M7V1B","RZAG140M7V1B"]
["Schalldruckpegel","Heizen","","Nom.","dBA","","","","52"]
["","Kühlung","","Nom.","dBA","","","","51"]
["Standardzubehör","Kabelbinder","","","","","","","2"]
["","Installationsanleitung","","","","","","","1"]
["","Kältemitteletikett für F-Gas-Bestimmungen","","","","","","","1"]
["","Allgemeine Schutzmaßnahmen","","","","","","","1"]
["","LOT 10 Energieeffizienzklasse","","","","","","","1"]
["Kältemittel","Charge","","","TCO2-Äquivalent","","","","2.53"]
["","GWP","","","","","","","675"]
["","Füllmenge","","","kg","","","","3.75"]
["","Typ","","","","","","","R-32"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","","","","9.52"]
["","Leitungslänge","Max.","AG – IG","M","","","","85"]
["","","System","Unbefüllt","M","","","","40"]
["","","","Äquivalent","M","","","","100"]
["","Gas","","AD","mm","","","","15.9"]
["","Niveauunterschied","IG - IG","Max.","M","","","","0.5"]
["","","IG - AG","Max.","M","","","","30.0"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","","","","Siehe Installationsanleitung"]
["Sound power level","Kühlung","","","dBA","","","","70"]
["","Heizen","","","dBA","","","","70 (1)"]
["Verdichter","Typ","","","","","","","Vollhermetischer Schwingverdichter"]
["Abmessungen","Maßeinheit","","Breite","mm","","","","940"]
["","","","Tiefe","mm","","","","320"]
["","","","Höhe","mm","","","","1,430"]
["Gewicht","Maßeinheit","","","kg","","","","92"]
["Power supply","Phase","","","","","","","1~"]
["","Frequenz","","","Hz","","","","50"]
["","Spannung","","","V","","","","220-240"]
["Hinweise","","","","","","","","(1) - Gemäß ENER Lot 21"]
["","","","","","","","","(2) - Europäisches/internationales Regelwerk bezüglich Grenzwerte: Oberschwingungsströme, verursacht von Geräten und Einrichtungen mit einem Eingangsstrom > 16 A und ≤ 75 A je Leiter, die zum Anschluss an öffentliche Niederspannungsnetze vorgesehen sind."]
["","","","","","","","","(3) - Ssc: Kurzschluss-Strom (Short-Circuit Power)"]
["","","","","","","","","(4) - Europäisches/internationales Regelwerk, indem zulässige Grenzwerte zu Oberschwingungsströmen festgelegt sind, die von an öffentlichen Niederspannungsnetzen angeschlossenen Anlagen und Geräten mit einem Eingangsstrom ≤ 16 A je Phase verursacht werden"]
["Abmessungen","Maßeinheit","","Höhe","mm","990","1430","1430"]
["","","","Breite","mm","940","940","940"]
["","","","Tiefe","mm","320","320","320"]
["Gewicht","Maßeinheit","","","kg","70","92","92"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C TK","-20","-20","-20"]
["","","","Max.","°C TK","52","52","52"]
["","Heizen","Umgebung","Min.","°C FK","-20","-20","-20"]
["","","","Max.","°C FK","18.0","18.0","18.0"]
["Schallleistungspegel","Kühlung","","","dBA","64","66","69"]
["Schalldruckpegel","Kühlung","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dBA","46","47","50"]
["","Heizen","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dBA","49","51","52"]
["Kältemittel","Typ","","","","R-32","R-32","R-32"]
["","Füllmenge","","","kg","2.95","3.75","3.75"]
["","GWP","","","","675","675","675"]
["","Füllmenge","","","tCO2Eq","1.99","2.53","2.53"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","9.52","9.52","9.52"]
["","Gas","","AD","mm","15.9","15.9","15.9"]
["","Leitungslänge","Max.","AG – IG","M","55","85","85"]
["","","System","Äquivalent","M","75","100","100"]
["","","","Unbefüllt","M","40","40","40"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","Siehe Installationsanleitung","Siehe Installationsanleitung","Siehe Installationsanleitung"]
["","Niveauunterschied","IG - AG","Max.","M","30.0","30.0","30.0"]
["","","IG - IG","Max.","M","0.5","0.5","0.5"]
["Standardzubehör","Installation manual","","","","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Tie-wraps","","","","2","2","2"]
["Stromversorgung","Phase","","","","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240","220-240"]
["Stromstärke&nbsp;– 50&nbsp;Hz","Stromstärke&nbsp;– 50&nbsp;Hz-=-Max. Amperezahl für Sicherung (MFA)-=-A","","","A","20","32","32"]
["Schallleistungspegel","Heizen","","","dBA","","","69 (1)"]
["Hinweise","","","","","","","(1) - Gemäß ENER Lot 21"]