{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":57,"n_cols":7,"rows_kept":57,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-C"]
[]
[]
[]
[]
["","","","","","RZQ200C7Y1B","RZQ250C7Y1B"]
["Abmessungen","Maßeinheit","","Höhe","mm","1,680"]
["","","","Breite","mm","930"]
["","","","Tiefe","mm","765"]
["Gewicht","Maßeinheit","","","kg","183.0"]
["Verdichter","Typ","","","","Hermetischer Scrollverdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°CTK","-5.0"]
["","","","Max.","°CTK","46.0"]
["","Heizen","Umgebung","Min.","°C FK","-15.0"]
["","","","Max.","°C FK","15.0"]
["Sound power level","Kühlung","","","dBA","78.0"]
["","Heizen","","","dBA","78.0"]
["Kältemittel","Typ","","","","R-410A"]
["","Füllmenge","","","kg","8.3"]
["","GWP","","","","2,087.5"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","9.52"]
["","Gas","","AD","mm","22.2"]
["","Leitungslänge","Max.","AG – IG","M","100"]
["","","System","Unbefüllt","M","30"]
["Standardzubehör","Installationsanleitung","","","","1"]
["","Verbindungsleitungen","","","","4"]
["Power supply","Phase","","","","3N~"]
["","Frequenz","","","Hz","50"]
["","Spannung","","","V","380-415"]
["Strom - 50 Hz","Max. Amperezahl für Sicherung (MFA)","","","A","25"]
["Hinweise","","","","","(1) - Stromversorgung für das FDQ-Innengerät erfolgt separat."]
["","","","","","(2) - Siehe separate Zeichnungen für die elektrischen Daten"]
["Abmessungen","Maßeinheit","","Höhe","mm","","1680"]
["","","","Breite","mm","","930"]
["","","","Tiefe","mm","","765"]
["Gewicht","Maßeinheit","","","kg","","184.0"]
["Verdichter","Typ","","","","","Hermetischer Scrollverdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°CTK","","-5.0"]
["","","","Max.","°CTK","","46.0"]
["","Heizen","Umgebung","Min.","°C FK","","-15.0"]
["","","","Max.","°C FK","","15.0"]
["Schallleistungspegel","Kühlung","","","dBA","","78.0"]
["","Heizen","","","dBA","","78.0"]
["Kältemittel","Typ","","","","","R-410A"]
["","Füllmenge","","","kg","","9.3"]
["","GWP","","","","","2087.5"]
["","Füllmenge","","","tCO2Eq","","19.4"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","","12.70"]
["","Gas","","AD","mm","","22.2"]
["","Leitungslänge","Max.","AG – IG","M","","100"]
["","","System","Unbefüllt","M","","30"]
["Standardzubehör","Installation manual","","","","","1"]
["","Connection pipes","","","","","4"]
["Stromversorgung","Phase","","","","","3N~"]
["","Frequenz","","","Hz","","50"]
["Spannungsversorgung","Spannung","","","V","","380-415"]
["Stromstärke&nbsp;– 50&nbsp;Hz","Stromstärke&nbsp;– 50&nbsp;Hz-=-Max. Amperezahl für Sicherung (MFA)-=-A","","","A","","25"]