{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQG-LV1L"]
[]
[]
[]
[]
["","","","","","RZQG71L9V1L"]
["Schallleistungspegel","Kühlung","","","dBA","64"]
["Abmessungen","Maßeinheit","","Höhe","mm","990"]
["","","","Breite","mm","940"]
["","","","Tiefe","mm","320"]
["Gewicht","Maßeinheit","","","kg","69.0"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C TK","-15"]
["","","","Max.","°C TK","50"]
["","Heizen","Umgebung","Min.","°C FK","-20"]
["","","","Max.","°C FK","16"]
["Schalldruckpegel","Kühlung","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dBA","48"]
["","Heizen","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dBA","50"]
["","Nachteinstellungsmodus","","Ebene 1","dBA","43"]
["Kältemittel","Füllmenge","","","kg","2.9"]
["","Füllmenge","","","tCO2Eq","6.10"]
["","GWP","","","","2087.5"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","m","50"]
["","Niveauunterschied","IG - AG","Max.","m","30.0"]
["","","IG - IG","Max.","m","0.5"]
["Standardzubehör","Installation manual","","","","1"]
["","Tie-wraps","","","","2"]
["Stromversorgung","Frequenz","","","Hz","50"]
["Hinweise","","","","","(1) - 3 mit Wiederbefüllung"]