{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":11,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXM-M"]
[]
[]
[]
[]
["","","","","","2AMXM40M2V1B","2AMXM40M3V1B","2AMXM40M4V1B","2AMXM50M2V1B","2AMXM50M4V1B","2AMXM50M3V1B"]
["Ventilateur","Débit d’air","Rafraîchissement","Extra lent","m³/min","30","","","34"]
["","","Chauffage","Très lent","m³/min","32","","","34"]
["Niveau de puissance sonore","Chauffage","","","dBA","","","62","","62"]
["","Rafraîchissement","","","dBA","","","60","","60"]
["Ventilateur","Débit d’air","Rafraîchissement","Extra lent","cfm","1059","","","1200"]
["","","Chauffage","Très lent","cfm","1130","","","1200"]
["Dimensions","Unité","","Hauteur","mm","550","550","550","550","550","550"]
["","","","Largeur","mm","765","765","765","765","765","765"]
["","","","Profondeur","mm","285","285","285","285","285","285"]
["Poids","Unité","","","kg","36","36","36","41","41","41"]
["Moteur de ventilateur","Vitesse","Rafraîchissement","Extra lent","tr/min","760","500","500","890","500","500"]
["","","Chauffage","Très lent","tr/min","820","320","320","890","500","500"]
["Compresseur","Type","","","","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","-10","","46.0","-10","46.0"]
["","","","Max.","°CBS","46","","-10","46","-10"]
["","Chauffage","Temp. ext.","Min.","°CBH","-15","","-15","-15","-15.0"]
["","","","Max.","°CBH","18","","18.0","18","18.0"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","","46","46","","48","48"]
["","","","Nom.","dBA","48","","","46"]
["","Chauffage","","Haut","dBA","","48","48","","50","50"]
["","","","Nom.","dBA","50","","","48"]
["Réfrigérant","","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Charge","","","kg","0.88","0.88","0.88","1.15","1.15","1.15"]
["","Charge","","","tCO2Eq","0.6","0.59","0.6","0.8","0.78","0.78"]
["","Réfrigérant-=-PRP","","","","675","675.0","675","675","675","675"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","20","20","20 (1)","20","20 (1)","20"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 20 m)","0,02 (pour longueur de tuyauterie supérieure à 20 m)","0,02 (pour longueur de tuyauterie supérieure à 20 m)","0,02 (pour longueur de tuyauterie supérieure à 20 m)","0,02 (pour longueur de tuyauterie supérieure à 20 m)","0,02 (pour longueur de tuyauterie supérieure à 20 m)"]
["","Dénivelé","UI - UE","Max.","m","15","15.0","15","15","15","15.0"]
["","","UI - UI","Max.","m","7.5","7.5","7.5","7.5","7.5","7.5"]
["","Longueur totale de tuyauterie","Système","Réel","m","30","30","30","30","30","30"]
["Accessoires standard","Installation manual","","","","Installation manual","1","1","1","1","1"]
["","Drain plug","","","","Drain plug","1","1","1","1","1"]
["","Screw bag","","","","Screw bag","1","1","1","1","1"]
["Alimentation électrique","Phase","","","","1~","1~","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50","50","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-230-240","220-230-240","220-240","220-230-240","220-230-240"]
["Remarques","","","","","","(1) - Par pièce","","","","(1) - Par pièce"]
["","","","","","","","(1) - Par pièce","","(1) - Par pièce"]
["","","","","","","","(2) - See separate drawing for operation range","","(2) - See separate drawing for operation range"]
["","","","","","","","(3) - See separate drawing for electrical data","","(3) - See separate drawing for electrical data"]
["","","","","","","","(4) - Contient des gaz à effet de serre fluorés.","","(4) - Contient des gaz à effet de serre fluorés."]
["Accessoires standard","Reducer assembly","","","","","","","1","1","1"]