{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-M9"]
[]
[]
[]
[]
["","","","","","2MXM50M3V1B9","2MXM50M2V1B9"]
["Dimensions","Unité","","Hauteur","mm","550","550"]
["","","","Largeur","mm","765","765"]
["","","","Profondeur","mm","285","285"]
["Poids","Unité","","","kg","41","41"]
["Moteur de ventilateur","Vitesse","Rafraîchissement","Extra lent","tr/min","500","500"]
["","","Chauffage","Très lent","tr/min","500","500"]
["Compressor","Type","","","","Compresseur swing hermétique","Compresseur swing hermétique"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","48","48"]
["","Chauffage","","Haut","dBA","50","50"]
["Réfrigérant","","","","","R-32","R-32"]
["","Charge","","","kg","1.15","1.15"]
["","Charge","","","tCO2Eq","0.78","0.8"]
["","Réfrigérant-=-PRP","","","","675","675.0"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","","20"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 20 m)","0,02 (pour longueur de tuyauterie supérieure à 20 m)"]
["","Dénivelé","UI - UE","Max.","m","15.0","15.0"]
["","","UI - UI","Max.","m","7.5","7.5"]
["","Longueur totale de tuyauterie","Système","Réel","m","30","30"]
["Accessoires standard","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Alimentation électrique","Phase","","","","1~","1~"]
["","Fréquence","","","Hz","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-230-240","220-230-240"]
["Remarques","","","","","(1) - Par pièce","(1) - Chaque unité D-AHU Professional peut être conçue selon vos besoins. Sélectionnez votre unité de traitement de l’air sur tools.daikinapplied.eu"]