{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":6,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMXF-A"]
[]
[]
[]
[]
["","","","","","3AMXF52A2V1B"]
["Dimensions","Unité","","Hauteur","mm","734"]
["","","","Largeur","mm","958"]
["","","","Profondeur","mm","340"]
["Poids","Unité","","","kg","57"]
["Moteur de ventilateur","Vitesse","Rafraîchissement","Extra lent","tr/min","420"]
["","","Chauffage","Très lent","tr/min","420"]
["Compresseur","Type","","","","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","-10"]
["","","","Max.","°CBS","46"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","46"]
["","Chauffage","","Nom.","dBA","47.0"]
["Réfrigérant","","","","","R-32"]
["","Charge","","","kg","1.8"]
["","Réfrigérant-=-Charge-=-Téq. CO₂","","","Téq. CO₂","1.22"]
["","Réfrigérant-=-PRP","","","","675.0"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","25 (1)"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 30 m)"]
["","Dénivelé","UI - UE","Max.","m","15.0"]
["","","UI - UI","Max.","m","7.5"]
["","Longueur totale de tuyauterie","Système","Réel","m","50"]
["Accessoires standard","Installation manual","","","","1"]
["","Drain cap","","","","3"]
["","Drain plug","","","","1"]
["","Reducer assembly","","","","1"]
["","Screw bag","","","","1"]
["Classe d'efficacité énergétique","","","","","A+++ ~ D"]
["Alimentation électrique","Phase","","","","1~"]
["","Fréquence","","","Hz","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240"]
["Remarques","","","","","(1) - Par pièce"]
["","","","","","(2) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","","(3) - Pour les données électriques, se reporter au schéma séparé."]
["","","","","","(4) - Contient des gaz à effet de serre fluorés."]