{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":14,"n_cols":4,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-C / ARXS-L3"]
[]
[]
[]
[]
["","","","ADEQ35C2VEB / ARXS35L3V1B"]
["Puissance frigorifique","Nom.","kW","3.40 (1)"]
["Puissance calorifique","Nom.","kW","4.00 (1)"]
["Remarques","","","(1) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°"]
["","","","(2) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]
["","","","(3) - DESP : montage = catégorie l : hors du champ d'application DESP en raison de l'article 1, élément 3.6 de la directive 97/23/CE"]
["","","","(4) - Valeur Ssc (=puissance de court-circuit) minimum : Équipement conforme à la norme EN 61000-3-2"]
["","","","(5) - Pour les données électriques, se reporter au schéma séparé."]
["","","","(6) - Contient des gaz à effet de serre fluorés."]