{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":58,"n_cols":7,"rows_kept":58,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R9"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B9","ARXM35R5V1B9"]
["Niveau de pression sonore","Chauffage","","Nom.","dBA","","49.0"]
["","Rafraîchissement","","Nom.","dBA","","49.0"]
["Accessoires standard","Bouchon d'évacuation","","","","","1"]
["","Manuel d'installation","","","","","1"]
["","Étiquette de charge de réfrigérant","","","","","1"]
["","Étiquettes multilingues de gaz à effet de serre fluorés","","","","","1"]
["","Précautions générales de sécurité","","","","","1"]
["Réfrigérant","Charge","","","TCO2Eq","","0.52"]
["","PRP","","","","","675"]
["","Charge","","","kg","","0.76"]
["","Type","","","","","R-32"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Max.","°CBS","","50 (4), 46 (5)"]
["","","","Min.","°CBS","","-10"]
["Raccordements de tuyauterie","Dénivelé","UI - UE","Max.","m","","15"]
["","Charge de réfrigérant supplémentaire","","","kg/m","","0,02 (pour longueur de tuyauterie supérieure à 10 m)"]
["Compresseur","Type","","","","","Compresseur swing hermétique"]
["Dimensions","Unité","","Largeur","mm","","840"]
["","","","Profondeur","mm","","350"]
["","","","Hauteur","mm","","552"]
["Poids","Unité","","","kg","","32"]
["Power supply","Phase","","","","","1~"]
["","Fréquence","","","Hz","","50"]
["","Tension","","","V","","220-240"]
["Remarques","","","","","(1) - Possible uniquement en combinaison avec ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Contient des gaz à effet de serre fluorés."]
["","","","","","(2) - Possible uniquement en combinaison avec ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","","","(3) - Pour les données électriques, se reporter au schéma séparé."]
["","","","","","","(4) - Possible uniquement en combinaison avec ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B"]
["","","","","","","(5) - Possible uniquement en combinaison avec ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B"]
["Dimensions","Unité","","Hauteur","mm","552"]
["","","","Largeur","mm","840"]
["","","","Profondeur","mm","350"]
["Poids","Unité","","","kg","32"]
["Compresseur","Type","","","","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","-10"]
["","","","Max.","°CBS","50 (4), 46 (5)"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","46.0"]
["","Chauffage","","Nom.","dBA","47.0"]
["Réfrigérant","","","","","R-32"]
["","Charge","","","kg","0.76"]
["","Charge","","","tCO2Eq","0.52"]
["","Réfrigérant-=-PRP","","","","675"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","20"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 10 m)"]
["","Dénivelé","UI - UE","Max.","m","15"]
["Accessoires standard","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","Drain plug","","","","1"]
["Alimentation électrique","Phase","","","","1~"]
["","Fréquence","","","Hz","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240"]