{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":7,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXQ-A"]
[]
[]
[]
[]
["","","","","","ARXQ25AMV1B","ARXQ35AMV1B"]
["Dimensions","Unité","","Hauteur","mm","550","550"]
["","","","Largeur","mm","740","740"]
["","","","Profondeur","mm","337","337"]
["Poids","Unité","","","kg","23.0","25.5"]
["Compresseur","Type","","","","Compresseur swing hermétique","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","10","10"]
["","","","Max.","°CBS","46","46"]
["","Chauffage","Temp. ext.","Min.","°CBH","-15","-15"]
["","","","Max.","°CBH","18","18"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","47.0","47.0"]
["Réfrigérant","","","","","R-32","R-32"]
["","Charge","","","kg","0.500","0.710"]
["","Charge","","","tCO2Eq","0.340","0.480"]
["","Réfrigérant-=-PRP","","","","675.0","675.0"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","15","15"]
["","Dénivelé","UI - UE","Max.","m","10.0","10.0"]
["Accessoires standard","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain plug","","","","1","1"]
["Alimentation électrique","Phase","","","","1~","1~"]
["","Fréquence","","","Hz","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240"]