{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":10,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L"]
[]
[]
[]
[]
["","","","","","ARXS25L2V1B","ARXS35L2V1B","ARXS50L2V1B","ARXS60L2V1B","ARXS71L2V1B"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","47","48"]
["","","","Nom.","dBA","","","","49","52"]
["","Rafraîchissement","","Haut","dBA","46","48"]
["","","","Nom.","dBA","","","","49","52"]
["Accessoires standard","Manuel d'installation","","","","1","1","","1","1"]
["","Bouchon d'évacuation","","","","1","1","","1","1"]
["","Étiquettes multilingues de gaz à effet de serre fluorés","","","","1","","","1","1"]
["","Étiquette de charge de réfrigérant","","","","1","","","1","1"]
["Réfrigérant","Charge","","","TCO2Eq","2.1","2.5"]
["","PRP","","","","2,087.5","2,087.5","","2,087.5","2,087.5"]
["","Charge","","","kg","1.0","1.2","","1.50","1.70"]
["","Type","","","","R-410A","R-410A","","R-410A","R-410A"]
["Moteur de ventil.","Vitesse","Rafraîchissement","Extra lent","tr/min","780","780"]
["","","Chauffage","Très lent","tr/min","740","740"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Max.","°CBS","46","46","","46","46"]
["","","","Min.","°CBS","10","10","","-10","-10"]
["","Chauffage","Extérieure","Max.","°CBH","18","18","","18","18"]
["","","","Min.","°CBH","-15","-15","","-15","-15"]
["Raccordements de tuyauterie","Dénivelé","UI - UE","Max.","m","15","15","","20.0","20.0"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)"]
["Sound power level","Rafraîchissement","","","dBA","","","","62","65"]
["","Chauffage","","","dBA","","","","62","65"]
["Compresseur","Type","","","","Compresseur swing hermétique","Compresseur swing hermétique","","Compresseur swing hermétique","Compresseur swing hermétique"]
["Dimensions","Unité","","Largeur","mm","765","765","","825","825"]
["","","","Profondeur","mm","285","285","","300","300"]
["","","","Hauteur","mm","550","550","","735","735"]
["Poids","Unité","","","kg","34","34","","47","47"]
["Ventilateur","Débit d'air","Chauffage","Très lent","cfm","904","904"]
["","","","Très lent","m³/min","25.6","25.6"]
["","","Rafraîchissement","Extra lent","m³/min","30.1","30.1"]
["","","","Extra lent","cfm","1,063","1,063"]
["Power supply","Phase","","","","1~","1~","","1~","1~"]
["","Fréquence","","","Hz","50","50","","50","50"]
["","Tension","","","V","220-240","220-240","","220-230-240","220-230-240"]
["Remarques","","","","","","","","(1) - Contient des gaz à effet de serre fluorés.","(1) - Contient des gaz à effet de serre fluorés."]
["","","","","","(1) - En cas de connexion à l’unité extérieure du système Multi, se reporter aux caractéristiques techniques de l’unité extérieure de type Multi à raccorder.","(1) - En cas de connexion à l’unité extérieure du système Multi, se reporter aux caractéristiques techniques de l’unité extérieure de type Multi à raccorder.","(1) - 220V"]
["","","","","","(2) - 220V","(2) - 220V","(2) - 230V"]
["","","","","","(3) - 230 V","(3) - 230 V","(3) - 240V"]
["","","","","","(4) - 240V","(4) - 240V"]
["","","","","","(5) - Contient des gaz à effet de serre fluorés.","(5) - Contient des gaz à effet de serre fluorés."]
["Ventilateur","Débit d’air","Rafraîchissement","Extra lent","m³/min","","","48.9"]
["","","Chauffage","Très lent","m³/min","","","43.1"]
["","","","Extra lent","cfm","","","1727"]
["","","Chauffage","Très lent","cfm","","","1522"]
["Dimensions","Unité","","Hauteur","mm","","","735"]
["","","","Largeur","mm","","","825"]
["","","","Profondeur","mm","","","300"]
["Poids","Unité","","","kg","","","47"]
["Moteur de ventilateur","Vitesse","Rafraîchissement","Extra lent","tr/min","","","670"]
["","","Chauffage","Très lent","tr/min","","","670"]
["Compresseur","Type","","","","","","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","","","10"]
["","","","Max.","°CBS","","","46"]
["","Chauffage","Temp. ext.","Min.","°CBH","","","-15"]
["","","","Max.","°CBH","","","18"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","","","48"]
["","Chauffage","","Haut","dBA","","","48"]
["Réfrigérant","","","","","","","R-410A"]
["","Charge","","","kg","","","1.7"]
["","Charge","","","tCO2Eq","","","3.5"]
["","Réfrigérant-=-PRP","","","","","","2087.5"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","","","30"]
["","Charge de réfrigérant supplémentaire","","","kg/m","","","0,02 (pour longueur de tuyauterie supérieure à 10 m)"]
["","Dénivelé","UI - UE","Max.","m","","","20"]
["Accessoires standard","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["Alimentation électrique","Phase","","","","","","1~"]
["","Fréquence","","","Hz","","","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","","","220-240"]