{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":86,"n_cols":11,"rows_kept":86,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATX-KV"]
[]
[]
[]
[]
["","","","","","ATX20K2V1B","ATX20K5V1B","ATX25K2V1B","ATX25K5V1B","ATX35K5V1B","ATX35K2V1B (Archived)"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","","","","","","43"]
["","","","Moyen","dBA","","","","","","35"]
["","","","Faible niveau sonore de fonctionnement","dBA","","","","","","26"]
["","","","Bas","dBA","","","","","","29"]
["","Rafraîchissement","","Moyen","dBA","","","","","","34"]
["","","","Faible niveau sonore de fonctionnement","dBA","","","","","","20"]
["","","","Bas","dBA","","","","","","27"]
["","","","Haut","dBA","","","","","","43"]
["Accessoires standard","Manuel d'installation","","","","","","","","","1"]
["","Manuel d’utilisation","","","","","","","","","1"]
["","Télécommande infrarouge","","","","","","","","","1"]
["","Piles sèches AA","","","","","","","","","2"]
["","Support de télécommande","","","","","","","","","1"]
["","Plaque de montage","","","","","","","","","1"]
["","Filtre purificateur d'air photocatalytique à apatite de titane","","","","","","","","","2"]
["","Vis de fixation d'unité intérieure","","","","","","","","","2"]
["Systèmes de contrôle","Wired remote control","","","","","","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","","","","","","ARC480A11"]
["Raccords de tuyauterie","Liquide","","DE","mm","","","","","","6.35"]
["","Gaz","","DE","mm","","","","","","9.50"]
["","Évacuation","","","","","","","","","18"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","","","","","","0.024"]
["","Chauffage","","Nom.","kW","","","","","","0.029"]
["Sound power level","Rafraîchissement","","","dBA","","","","","","58"]
["","Chauffage","","","dBA","","","","","","58"]
["Dimensions","Unité","","Largeur","mm","","","","","","770"]
["","","","Profondeur","mm","","","","","","225"]
["","","","Hauteur","mm","","","","","","286"]
["Caisson","Couleur","","","","","","","","","Blanc"]
["Poids","Unité","","","kg","","","","","","9.0"]
["Power supply","Phase","","","","","","","","","1~"]
["","Fréquence","","","Hz","","","","","","50"]
["","Nom","","","","","","","","","V1"]
["","Tension","","","V","","","","","","220-240"]
["Remarques","","","","","","","","","","(1) - SL : Très faible niveau sonore de ventilation (réglage du débit d’air)"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.018","0.018","0.02","0.02","0.024"]
["","Chauffage","","Nom.","kW","0.022","0.022","0.023","0.023","0.029"]
["Caisson","Couleur","","","","Blanc","Blanc","Blanc","Blanc","Blanc"]
["Dimensions","Unité","","Hauteur","mm","286","286","286","286","286"]
["","","","Largeur","mm","770","770","770","770","770"]
["","","","Profondeur","mm","225","225","225","225","225"]
["Poids","Unité","","","kg","8.5","8.5","8.5","8.5","9"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","9.9","9.9","10.4","10.4","11.8"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","7.8","7.8","8","8","8.2"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","5.8","5.8","6.1","6.1","6.3"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.8","4.8","4.8","4.8","4.9"]
["","","Chauffage","Haut","m³/min","10.9","10.9","11.1","11.1","12.8"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","8.5","8.5","8.5","8.5","8.5"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","6.4","6.4","6.7","6.7","6.9"]
["","","","Faible niveau sonore de fonctionnement","m³/min","5.2","5.2","5.2","5.2","5.2"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","55","55","55","55","58"]
["","Chauffage","","","dBA","55","55","55","55","58"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","39","39","40","40","43"]
["","Refroidissement","","Moyen","dBA","33","33","33","33","34"]
["","","","Bas","dBA","25","25","26","26","27"]
["","","","Faible niveau sonore de fonctionnement","dBA","20","20","20","20","20"]
["","Chauffage","","Haut","dBA","39","39","40","40","43"]
["","","","Moyen","dBA","34","34","34","34","35"]
["","","","Bas","dBA","28","28","28","28","29"]
["","","","Faible niveau sonore de fonctionnement","dBA","23","23","23","23","26"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gaz","","DE","mm","9.5","9.5","9.5","9.5","9.5"]
["","Évacuation","","","","18","18","18","18","18"]
["Systèmes de contrôle","Infrared remote control","","","","ARC480A11","ARC480A11","","","ARC480A11"]
["Systèmes de commande","Télécommande câblée","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Accessoires standard","Installation manual","","","","1","1","1","1","1"]
["","AA dry-cell batteries","","","","2","","2"]
["","Operation manual","","","","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1"]
["Alimentation électrique","Nom","","","","V1","V1","V1","V1","V1"]
["","Phase","","","","1~","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240","220-240","220-240","220-240"]
["Accessoires standard","AAA dry-cell batteries","","","","","2","","2","2"]
["Systèmes de commande","Télécommande infrarouge","","","","","","ARC480A11","ARC480A11"]
["Accessoires standard","Titanium apatite photocatalytic air purification filter","","","","","","2"]