{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":10,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXC-C / ARXC-C"]
[]
[]
[]
[]
["","","","","ATXC20CV1B / ARXC20CV1B","ATXC25CV1B / ARXC25CV1B","ATXC35CV1B / ARXC35CV1B","ATXC50CV1B / ARXC50CV1B","ATXC60CV1B / ARXC60CV1B","ATXC71CV1B / ARXC71CV1B"]
["Puissance frigorifique","Min.","","kW","1.3","1.3","1.3","1.4","1.8","2.3"]
["","Max.","","kW","3.0","3.0","4.0","6.2","7.0","7.3"]
["Rafraîchissement de l'air ambiant","SEER","","","6.81","6.74","6.78","6.40","6.38","5.25"]
["","Consommation d’énergie annuelle","","kWh/a","107","133","178","278","341","464"]
["","Puissance","Pdesign","kW","2.08","2.57","3.44","5.08","6.21","6.96"]
["","Classe d’efficacité énergétique","","","A++","A++","A++","A++","A++","A"]
["Chauffage des locaux (climat tempéré)","Puissance","Pdesign","kW","1.87","2.23","2.24","3.90","4.10","6.35"]
["","SCOP/A","","","4.39","4.41","4.26","4.37","4.19","3.81"]
["","Classe d’efficacité énergétique","","","A+","A+","A+","A+","A+","A"]
["","Consommation d’énergie annuelle","","kWh/a","595","707","736","1,250","1,373","2,334"]
["Efficacité nominale","EER","","","3.33","3.30","3.30","3.25","3.25","2.95"]
["","COP","","","3.73","3.76","3.72","3.71","3.71","3.21"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","A","A","A","A","C"]
["","","Chauffage","","A","A","A","A","A","C"]
["Puissance calorifique","Min.","","kW","1.30","1.30","1.30","1.36","1.48","2.30"]
["","Max.","","kW","4.00","4.00","4.80","6.60","8.00","9.00"]