{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":80,"n_cols":9,"rows_kept":80,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-C"]
[]
[]
[]
[]
["","","","","","ATXF20C5V1B","ATXF25C5V1B","ATXF35C5V1B","ATXF42C5V1B"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","39.0","40.0","","44.0"]
["","","","Moyen","dBA","34.0","34.0","","34.0"]
["","","","Faible niveau sonore de fonctionnement","dBA","21.0","21.0","","22.0"]
["","","","Bas","dBA","28.0","28.0","","28.0"]
["","Rafraîchissement","","Moyen","dBA","33.0","33.0","","36.0"]
["","","","Faible niveau sonore de fonctionnement","dBA","20.0","20.0","","22.0"]
["","","","Bas","dBA","25.0","26.0","","30.0"]
["","","","Haut","dBA","39.0","40.0","","45.0"]
["Accessoires standard","Manuel d'installation","","","","1","1","","1"]
["","Manuel d’utilisation","","","","1","1","","1"]
["","Piles","","","","1","1","","1"]
["","Télécommande infrarouge","","","","1","1","","1"]
["","Piles sèches AAA","","","","2","2","","2"]
["","Support de télécommande","","","","1","1","","1"]
["","Plaque de montage","","","","1","1","","1"]
["","Vis de fixation d'unité intérieure","","","","2","2","","2"]
["Systèmes de contrôle","Wired remote control","","","","BRC073A1","BRC073A1","","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","","ARC470A1"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","6.35","","6.35"]
["","Gaz","","DE","mm","9.50","9.50","","9.50"]
["","Évacuation","","","","18","18","","18"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.023","0.023","","0.040"]
["","Chauffage","","Nom.","kW","0.023","0.023","","0.040"]
["Sound power level","Rafraîchissement","","","dBA","53.0","54.0","","59.0"]
["","Chauffage","","","dBA","55.0","55.0","","59.0"]
["Dimensions","Unité","","Largeur","mm","770","770","","770"]
["","","","Profondeur","mm","225","225","","225"]
["","","","Hauteur","mm","286","286","","286"]
["Caisson","Couleur","","","","Blanc","Blanc","","Blanc"]
["Poids","Unité","","","kg","8.00","8.00","","9.00"]
["Power supply","Phase","","","","1~","1~","","1~"]
["","Fréquence","","","Hz","50","50","","50"]
["","Tension","","","V","220-440","220-440","","220-440"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","","","0.029"]
["","Chauffage","","Nom.","kW","","","0.029"]
["Caisson","Couleur","","","","","","Blanc"]
["Dimensions","Unité","","Hauteur","mm","","","286"]
["","","","Largeur","mm","","","770"]
["","","","Profondeur","mm","","","225"]
["Poids","Unité","","","kg","","","8.5"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","","","11.8"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","","","8"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","","","6.4"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","","4.4"]
["","","Chauffage","Haut","m³/min","","","11.9"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","","","8.6"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","","","6.5"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","","5.3"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","","","54"]
["","Chauffage","","","dBA","","","56"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","","","43"]
["","Refroidissement","","Moyen","dBA","","","34"]
["","","","Bas","dBA","","","27"]
["","","","Faible niveau sonore de fonctionnement","dBA","","","20"]
["","Chauffage","","Haut","dBA","","","40"]
["","","","Moyen","dBA","","","35"]
["","","","Bas","dBA","","","29"]
["","","","Faible niveau sonore de fonctionnement","dBA","","","21"]
["Raccords de tuyauterie","Liquide","","DE","mm","","","6.35"]
["","Gaz","","DE","mm","","","9.5"]
["","Évacuation","","","","","","18"]
["Systèmes de commande","Télécommande infrarouge","","","","","","ARC470A1"]
["","Télécommande câblée","","","","","","BRC073A1"]
["Accessoires standard","Installation manual","","","","","","1"]
["","AAA dry-cell batteries","","","","","","2"]
["","Operation manual","","","","","","1"]
["","Batteries","","","","","","1"]
["","Indoor unit fixing screws","","","","","","2"]
["","Infrared remote control","","","","","","1"]
["","Mounting plate","","","","","","1"]
["","Remote control holder","","","","","","1"]
["Alimentation électrique","Phase","","","","","","1~"]
["","Fréquence","","","Hz","","","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","","","220-440"]