{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-F / RXF-D"]
[]
[]
[]
[]
["","","","","ATXF50F5V1B / RXF50D5V1B","ATXF50F5V1B / RXF50D6V1B"]
["Unité extérieure","","","","RXF50D5V1B","RXF50D6V1B"]
["Puissance frigorifique","Min.","","kW","1.70","1.70"]
["","Nom.","","kW","5.00","5.00"]
["","Max.","","kW","6.00","6.00"]
["Puissance calorifique","Puissance calorifique-=-Min.-=-kW","","kW","1.70","1.70"]
["","Nom.","","kW","6.00","6.00"]
["","Max.","","kW","7.70","7.70"]
["Efficacité nominale","EER","","","3.30","3.30"]
["","COP","","","3.71","3.71"]
["","Consommation énergétique annuelle","","kWh","283","283"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","A"]
["","","Chauffage","","A","A"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","A++","A++"]
["","Puissance","Pdesign","kW","5.00","5.00"]
["","SEER","","","6.18","6.18"]
["","Consommation d’énergie annuelle","","kWh/a","283","283"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","A+","A+"]
["","Puissance","Pdesign","kW","4.60","4.60"]
["","SCOP/A","","","4.03","4.03"]
["","Pdh Puissance calorifique à -10°","","kW","4.06","4.06"]
["","Consommation d’énergie annuelle","","kWh/a","1598","1598"]
["Remarques","","","","(1) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m.","(1) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]