{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":70,"n_cols":9,"rows_kept":70,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXN-NB9"]
[]
[]
[]
[]
["","","","","","ATXN25NV1B9","ATXN35NV1B9","ATXN50NV1B9","ATXN60NV1B9"]
["Niveau de pression sonore","Rafraîchissement","","Faible niveau sonore de fonctionnement","dBA","21","22","","33"]
["","","","Très élevé","dBA","41","42","","46"]
["","","","Bas","dBA","29","30","","37"]
["","","","Haut","dBA","40","41","","43"]
["Accessoires standard","Manuel d'installation","","","","1","1","","1"]
["","Manuel d’utilisation","","","","1","1","","1"]
["","Télécommande infrarouge","","","","1","1","","1"]
["","Piles","","","","Piles","Piles","","Piles"]
["","Support de télécommande","","","","1","1","","1"]
["","Plaque de montage","","","","1","1","","1"]
["","Filtres à apatite de titane","","","","Filtres à apatite de titane","Filtres à apatite de titane","","Filtres à apatite de titane"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","6.35","","6.35"]
["","Gaz","","DE","mm","9.50","9.50","","15.90"]
["","Évacuation","","","","16.5","16.5","","16.5"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","693.00","1,060.00","","1,931.00"]
["","Chauffage","","Nom.","kW","700.00","950.00","","1,680.00"]
["Sound power level","Rafraîchissement","","","dBA","53","54","","61"]
["Dimensions","Unité","","Largeur","mm","859","859","","1,124"]
["","","","Profondeur","mm","209","209","","237"]
["","","","Hauteur","mm","288","288","","310"]
["Caisson","Matériau","","","","Polystyrène à fort impact","Polystyrène à fort impact","","Polystyrène à fort impact"]
["","Couleur","","","","Blanc","Blanc","","Blanc"]
["Poids","Unité","","","kg","9.0","9.0","","14.0"]
["Power supply","Phase","","","","1~","1~","","1~"]
["","Fréquence","","","Hz","50","50","","50"]
["","Nom","","","","V1","V1","","V1"]
["","Tension","","","V","220-240","220-240","","220-240"]
["Remarques","","","","","(1) - Toutes les unités sont testées et conformes à la norme ISO5151 (unité non gainée) ou ISO13253 (unité gainée)","(1) - Toutes les unités sont testées et conformes à la norme ISO5151 (unité non gainée) ou ISO13253 (unité gainée)","","(1) - Toutes les unités sont testées et conformes à la norme ISO5151 (unité non gainée) ou ISO13253 (unité gainée)"]
["","","","","","(2) - Toutes les caractéristiques techniques sont sujettes à modification par le fabricant sans préavis.","(2) - Toutes les caractéristiques techniques sont sujettes à modification par le fabricant sans préavis.","","(2) - Toutes les caractéristiques techniques sont sujettes à modification par le fabricant sans préavis."]
["Ventilateur","Débit d'air","Rafraîchissement","Nom.","m³/min","","","13.30"]
["","","Chauffage","Nom.","m³/min","","","13.30"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","","","1668"]
["","Chauffage","","Nom.","kW","","","1550"]
["Caisson","Couleur","","","","","","Blanc"]
["","Matériau","","","","","","Polystyrène à fort impact"]
["Dimensions","Unité","","Hauteur","mm","","","310"]
["","","","Largeur","mm","","","1124"]
["","","","Profondeur","mm","","","237"]
["Poids","Unité","","","kg","","","14"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","","","15"]
["","","","Bas","m³/min","","","11.8"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","","10.6"]
["","","Chauffage","Haut","m³/min","","","15.3"]
["","","","Bas","m³/min","","","11.8"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","","10.6"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","","","55"]
["Niveau de pression sonore","Rafraîchissement","","Très élevé","dBA","","","44"]
["","","","Haut","dBA","","","40"]
["","","","Bas","dBA","","","35"]
["","","","Faible niveau sonore de fonctionnement","dBA","","","32"]
["Raccords de tuyauterie","Liquide","","DE","mm","","","6.35"]
["","Gaz","","DE","mm","","","12.7"]
["","Évacuation","","","","","","16.5"]
["Accessoires standard","Installation manual","","","","","","1"]
["","Wireless remote control","","","","","","1"]
["","Titanium apatite filters","","","","","","Titanium apatite filters"]
["","Operation manual","","","","","","1"]
["","Batteries","","","","","","Batteries"]
["","Mounting plate","","","","","","1"]
["","Remote control holder","","","","","","1"]
["Alimentation électrique","Nom","","","","","","V1"]
["","Phase","","","","","","1~"]
["","Fréquence","","","Hz","","","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","","","220-240"]