{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-K3 / ARXP-K3"]
[]
[]
[]
[]
["","","","","ATXP20K3V1B / ARXP20K3V1B","ATXP25K3V1B / ARXP25K3V1B","ATXP35K3V1B / ARXP35K3V1B"]
["Puissance frigorifique","Nom.","","kW","","2.50","3.50"]
["Efficacité nominale","EER","","","","3.79","3.45"]
["","COP","","","","4.36","4.02"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","","A","A"]
["","","Chauffage","","","A","A"]
["Puissance calorifique","Nom.","","kW","","3.00","4.00"]
["Remarques","","","","","(1) - Rafraîchissement : T2 : temp. intérieure 26,6°C BS, 19,4°C BH ; temp. extérieure 48°C BS [Btu/h/W]","(1) - Rafraîchissement : T2 : temp. intérieure 26,6°C BS, 19,4°C BH ; temp. extérieure 48°C BS [Btu/h/W]"]
["","","","","","(2) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m.","(2) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m."]
["","","","","","(3) - Pour les données électriques, se reporter au schéma séparé.","(3) - Pour les données électriques, se reporter au schéma séparé."]
["Unité extérieure","","","","ARXP20K3V1B"]
["Puissance frigorifique","Nom.","","kW","2.00"]
["Puissance calorifique","Nom.","","kW","2.50"]
["Efficacité nominale","EER","","","3.98"]
["","COP","","","4.77"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A"]
["","","Chauffage","","A"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","A++"]
["","Puissance","Pdesign","kW","2.00"]
["","SEER","","","6.75"]
["","Consommation d’énergie annuelle","","kWh/a","104"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","A++"]
["","Puissance","Pdesign","kW","2.20"]
["","SCOP/A","","","4.64"]
["","Pdh Puissance calorifique à -10°","","kW","2.19"]
["","Consommation d’énergie annuelle","","kWh/a","664"]