{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":7,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXQ-A"]
[]
[]
[]
[]
["","","","","","ATXQ25AMV1B","ATXQ35AMV1B"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.023","0.025"]
["","Chauffage","","Nom.","kW","0.027","0.031"]
["Caisson","Couleur","","","","Blanc","Blanc"]
["Dimensions","Unité","","Hauteur","mm","291","291"]
["","","","Largeur","mm","770","770"]
["","","","Profondeur","mm","232","232"]
["Poids","Unité","","","kg","9","9"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","10.2","10.5"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","8.1","8.5"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","6.5","7"]
["","","","Faible niveau sonore de fonctionnement","m³/min","5","6"]
["","","Chauffage","Haut","m³/min","11.1","12"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","9.6","10"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","8.1","8.3"]
["","","","Faible niveau sonore de fonctionnement","m³/min","6.8","6.9"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","55","55"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","40","41"]
["","Refroidissement","","Moyen","dBA","34","35"]
["","","","Bas","dBA","26","28"]
["","","","Faible niveau sonore de fonctionnement","dBA","23","24"]
["","Chauffage","","Haut","dBA","40","42"]
["","","","Moyen","dBA","34","35"]
["","","","Bas","dBA","29","30"]
["","","","Faible niveau sonore de fonctionnement","dBA","25","25"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","6.35"]
["","Gaz","","DE","mm","9.5","9.5"]
["","Évacuation","","","","18","18"]
["Systèmes de commande","Télécommande infrarouge","","","","ARC470A1","ARC470A1"]
["Accessoires standard","Installation manual","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Infrared remote control","","","","1","1"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Alimentation électrique","Phase","","","","1~","1~"]
["","Fréquence","","","Hz","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240"]