{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":8,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXV-AB / ARXV-AB"]
[]
[]
[]
[]
["","","","","ATXV25AV1B / ARXV25AV1B","ATXV35AV1B / ARXV35AV1B","ATXV50AV1B / ARXV50AV1B","ATXV60AV1B / ARXV60AV1B"]
["Puissance frigorifique","Min.","","kW","0.6","0.6","1.26","2.53"]
["","Max.","","kW","3.2","3.9","6","6.8"]
["","Nom.","","kW","2.65","3.4","5.2","6.25"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","445","665","835","1,075"]
["","EER","","","2.98","2.56","3.11","2.91"]
["","COP","","","3.11","3.12","3.23","2.96"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","C","E","B","C"]
["","","Chauffage","","D","D","C","D"]
["Puissance calorifique","Nom.","","kW","2.8","3.84","5.65","6.75"]
["","Min.","","kW","0.8","0.88","1.12","2.53"]
["","Max.","","kW","3.6","4.4","6.8","7.6"]
["Remarques","","","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]
["","","","","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°"]