{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":9,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXV-AB"]
[]
[]
[]
[]
["","","","","","ATXV25AV1B","ATXV35AV1B","ATXV50AV1B","ATXV60AV1B"]
["Niveau de pression sonore","Rafraîchissement","","Faible niveau sonore de fonctionnement","dBA","28","","35","39"]
["","","","Bas","dBA","34","","40","42"]
["","","","Haut","dBA","41","","48","51"]
["","","","Nom.","dBA","39","","43","47"]
["Systèmes de contrôle","Infrared remote control","","","","ARC470A21","","ARC470A21","ARC470A21"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","","6.35","6.35"]
["","Gaz","","DE","mm","9.52","","12.7","15.9"]
["Sound power level","Rafraîchissement","","","dBA","50","","53","57"]
["Dimensions","Unité","","Largeur","mm","845","","940","1,007"]
["","","","Profondeur","mm","180","","200","219"]
["","","","Hauteur","mm","275","","298","315"]
["Poids","Unité","","","kg","9","","12","14"]
["Power supply","Phase","","","","1~","","1~","1~"]
["","Fréquence","","","Hz","50","","50","50"]
["","Tension","","","V","220-240","","220-240","220-240"]
["Ventilateur","Débit d'air","Rafraîchissement","Nom.","m³/min","","8.3"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","","40"]
["Dimensions","Unité","","Hauteur","mm","","275"]
["","","","Largeur","mm","","845"]
["","","","Profondeur","mm","","180"]
["Poids","Unité","","","kg","","9"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","","9.7"]
["","","","Bas","m³/min","","6.7"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","5"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","","51"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","","42"]
["","","","Bas","dBA","","35"]
["","","","Faible niveau sonore de fonctionnement","dBA","","30"]
["Raccords de tuyauterie","Liquide","","DE","mm","","6.35"]
["","Gaz","","DE","mm","","9.52"]
["Systèmes de commande","Télécommande infrarouge","","","","","ARC470A21"]
["Alimentation électrique","Phase","","","","","1~"]
["","Fréquence","","","Hz","","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","","220-240"]