{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BR00000749"]
[]
[]
[]
[]
["","","","","","BR00000749."]
["Type","","","","","Purificateur d'air"]
["Application","","","","","Type console carrossée"]
["Puissance","m³/min","","","","33.33"]
["Caisson","Couleur","","","","Finition en acier galvanisé peint"]
["Dimensions","Unité","","Hauteur","mm","1628"]
["","","","Largeur","mm","720"]
["","","","Profondeur","mm","770"]
["Poids","Unité","","","kg","150"]
["Surface applicable","m²","","","","133"]
["Mode purification","Puissance absorbée","","GV","kW","0.379"]
["Niveau de pression sonore","Mode purification","","Haut","dBA","55.9"]
["Ventilateur","Débit d'air","Mode purification","Turbo","m³/h","2300"]
["","","","Haut","m³/h","2000"]
["Méthode de collecte des poussières","","","","","Préfiltre RedPleat, ISO Coarse 70 % 592 x 592 x 45, filtration HEPA H14"]
["Méthode de filtrage des bactéries","","","","","Astrocel III HEPA H14, A39A05C9S2R3"]
["Dispositifs de sécurité","Élément","","01","","Interrupteur de sécurité (arrêt du fonctionnement à l'ouverture de la porte arrière)"]
["Accessoires standard","Prefilter selected","","","","1"]
["","HEPA filter selected","","","","1"]
["","Quick Start and Maintenance Guide","","","","1"]
["","Installation and Operation Manual available for download","","","","1"]
["Cordon d'alimentation","m","","","","3"]
["Alimentation électrique","Phase","","","","1~"]
["","Fréquence","","","Hz","50/60"]
["","Alimentation électrique-=-Tension-=-V","","","V","230"]
["Courant de fonctionnement","Mode purification","","Haut","A","1.73"]