{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1HHDW"]
[]
[]
[]
[]
["","","","","BRC1HHDAW (Archived)"]
["Caisson","Couleur","","","Blanc"]
["Casing","Couvercle de boutons","","","Non"]
["Caisson","DEL de fonctionnement","Couleur","","Indicateur d'état bleu"]
["Dimensions","Unité","Hauteur","mm","85"]
["","","Largeur","mm","85"]
["","","Profondeur","mm","25"]
["","Unité emballée","Hauteur","mm","50"]
["","","Largeur","mm","217"]
["","","Profondeur","mm","161"]
["Poids","Unité","","kg","0.110"]
["","Unité emballée","","kg","0.317"]
["Emballage","Matériau","","","Carton"]
["","Poids","","kg","0.0850"]
["Écran LCD","Type","","","100 x 150 points"]
["","Dimensions","Hauteur","mm","40.7"]
["","","Largeur","mm","28.0"]
["Écran LCD","Rétroéclairage","Couleur","","Blanc"]
["Température extérieure","Fonctionnement","Min.","°C","-10"]
["","","Max.","°C","52"]
["","Stockage","Min.","°C","-20"]
["","","Max.","°C","70"]
["","Température extérieure-=-Humidité relative <-=-%","","%","95"]
["Systèmes de contrôle","Classe de contrôle de température","","","VI"]
["","Contribution à l'efficacité saisonnière du chauffage de l'air ambiant","","%","4.0"]
["Raccords de câblage","Longueur de câble","Raccords de câblage-=-Longueur de câble-=-Max.-=-m","m","500"]