{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":6,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BSV4Q-PV"]
[]
[]
[]
[]
["","","","","","BSV4Q100PV1"]
["Accessoires standard","Manuel d'installation","","","","Manuel d'installation"]
["","Tuyau fourni","","","","Tuyau fourni"]
["","Protection de tuyau isolante","","","","Protection de tuyau isolante"]
["","Attaches","","","","Attaches"]
["Nombre maximum d'unités intérieures connectables par embranchement","","","","","6"]
["Nombre maximum d'unités intérieures connectables","","","","","24"]
["Piping connections","Unité extérieure","Liquide","Type","","Raccord brasé"]
["","","","DE","mm","12.7"]
["","","Refoulement de gaz","Type","","Raccord brasé"]
["","","","DE","mm","19.1"]
["","","Gaz","Type","","Raccord brasé"]
["","","","DE","mm","28.6"]
["","Unité intérieure","Gaz","Type","","Raccord brasé"]
["","","","DE","mm","15.9"]
["","","Liquide","DE","mm","9.5"]
["","","","Type","","Raccord brasé"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.020"]
["","Chauffage","","Nom.","kW","0.020"]
["Indice de puissance maximum d'unités intérieures connectables par embranchement","","","","","100"]
["Dimensions","Unité","","Largeur","mm","1,053"]
["","","","Profondeur","mm","635"]
["","","","Hauteur","mm","209"]
["Poids","Unité","","","kg","60"]
["Nombre d'embranchements","","","","","4"]
["Maximum capacity index of connectable indoor units","","","","","400"]
["Power supply","Phase","","","","1~"]
["","Fréquence","","","Hz","50"]
["","Tension","","","V","220-240"]
["","Nom","","","","V1"]
["Remarques","","","","","(1) - En cas de raccordement d’une unité intérieure de type 20~50, coller à la taille du tuyau sur site à l’aide du tuyau fourni. Le raccordement entre le tuyau fourni et le tuyau sur site doit être brasé."]
["","","","","","(2) - Si le diamètre de joint n'est pas adapté au côté triple tuyauterie, l'utilisation d'un réducteur est nécessaire (à fournir sur site)."]
["","","","","","(3) - Isolants nécessaires (à fournir sur site) pour le côté à triple tuyauterie"]
["","","","","","(4) - Plage de tension : les unités sont conçues pour fonctionner sur des systèmes électriques dont la tension d'alimentation est comprise dans les limites de la plage de tension précisées."]
["","","","","","(5) - La variation maximum admissible de la plage de tension entre phases est de 2 %."]
["","","","","","(6) - MCA/MFA : MCA = 1,25 x FLA"]
["","","","","","(7) - MFA < 4 x FLA"]
["","","","","","(8) - Calibre de fusible standard immédiatement inférieur : minimum 15A."]
["","","","","","(9) - Choisir la taille de câble en fonction de la valeur MCA"]
["","","","","","(10) - En lieu et place d'un fusible, utiliser un disjoncteur."]