{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":5,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXF-C / 3MXF-A9"]
[]
[]
[]
[]
["","","","","CTXF20C5V1B / CTXF20C5V1B / CTXF20C5V1B / 3MXF52A2V1B9"]
["Puissance frigorifique","Min.","","kW","1.80"]
["","Max.","","kW","7.00"]
["","Nom.","","kW","5.20"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","634"]
["","EER","","","4.10"]
["","COP","","","3.93"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A"]
["","","Chauffage","","A"]
["Puissance calorifique","Nom.","","kW","6.80"]
["","Min.","","kW","1.30"]
["","Max.","","kW","8.00"]