{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":8,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXF-F"]
[]
[]
[]
[]
["","","","","","CTXF20F5V1B","CTXF25F5V1B","CTXF35F5V1B"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.023","0.023","0.029"]
["","Chauffage","","Nom.","kW","0.023","0.023","0.023"]
["Caisson","Couleur","","","","Blanc","Blanc","Blanc"]
["Dimensions","Unité","","Hauteur","mm","286","286","286"]
["","","","Largeur","mm","770","770","770"]
["","","","Profondeur","mm","225","225","225"]
["Poids","Unité","","","kg","8.5","8.5","9"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","9.8","9.8","10.9"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","8","8","7"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","6","6","5.7"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.3","4.3","4.6"]
["","","Chauffage","Haut","m³/min","10.4","10.4","9.3"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","8.3","8.4","7.5"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","6.2","6.4","6"]
["","","","Faible niveau sonore de fonctionnement","m³/min","5.3","5.3","5.2"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","53","54","54"]
["","Chauffage","","","dBA","55","55","56"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","39","40","56"]
["","Refroidissement","","Moyen","dBA","33","33"]
["","","","Bas","dBA","25","26"]
["","","","Faible niveau sonore de fonctionnement","dBA","20","20"]
["","Chauffage","","Haut","dBA","39","40","40"]
["","","","Moyen","dBA","33","34","35"]
["","","","Bas","dBA","28","28","29"]
["","","","Faible niveau sonore de fonctionnement","dBA","21","21","21"]
["Raccords de tuyauterie","Liquide","","DE","mm","6","6","6"]
["","Gaz","","DE","mm","9.5","9.5","9.5"]
["","Évacuation","","","","18","18","18"]
["Systèmes de commande","Télécommande infrarouge","","","","ARC480A93","ARC480A93","ARC480A93"]
["","Télécommande câblée","","","","BRC073A1","BRC073A1","BRC073A1"]
["Accessoires standard","Installation manual","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Infrared remote control","","","","1","1","1"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Alimentation électrique","Phase","","","","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-440","220-440","220-440"]
["Remarques","","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Rafraîchissement: temp. intérieure 27°CBS, 19°CBH; temp. extérieure 35°CBS; longueur équivalente de tuyauterie : 5m; dénivelé: 0m","(1) - Rafraîchissement: temp. intérieure 27°CBS, 19°CBH; temp. extérieure 35°CBS; longueur équivalente de tuyauterie : 5m; dénivelé: 0m"]
["","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","(2) - Chauffage: temp. intérieure 20°CBS; temp. extérieure 7°CBS, 6°CBH ; tuyauterie équivalente de réfrigérant : 5m (horizontale)","(2) - Chauffage: temp. intérieure 20°CBS; temp. extérieure 7°CBS, 6°CBH ; tuyauterie équivalente de réfrigérant : 5m (horizontale)"]
["","","","","","(3) - See separate drawing for electrical data","(3) - Pour les données électriques, se reporter au schéma séparé.","(3) - Pour les données électriques, se reporter au schéma séparé."]