{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":28,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CYA-DK-F"]
[]
[]
[]
[]
["","","","","CYAL100DK125FB","CYAL100DK125FS","CYAM100DK80FB","CYAM100DK80FS","CYAS100DK80FB","CYAS100DK80FS","CYAL150DK200FB","CYAL150DK200FS","CYAM150DK80FB","CYAM150DK80FS","CYAS150DK80FB","CYAS150DK80FS","CYAL200DK250FB","CYAL200DK250FS","CYAM200DK100FB","CYAM200DK100FS","CYAS200DK100FB","CYAS200DK100FS","CYAL250DK250FB","CYAL250DK250FS","CYAM250DK140FB","CYAM250DK140FS","CYAS250DK140FB","CYAS250DK140FS"]
["Puissance absorbée","Ventilation seule","Nom.","kW","0.48","0.48","0.27","0.27","0.1426","0.1426","0.7245","0.7245","0.4","0.4","0.2139","0.2139","0.96","0.96","0.53","0.53","0.28","0.28","1.2","1.2","0.67","0.67","0.36","0.36"]
["","Chauffage","Nom.","kW","0.48","0.48","0.27","0.27","0.1426","0.1426","0.7245","0.7245","0.4","0.4","0.2139","0.2139","0.96","0.96","0.53","0.53","0.28","0.28","1.2","1.2","0.67","0.67","0.36","0.36"]
["Largeur de porte","Max.","","m","1","1","1","1","1","1","1.5","1.5","1.5","1.5","1.5","1.5","2","2","2","2","2","2","2.5","2.5","2.5","2.5","2.5","2.5"]
["Hauteur de porte","Max.","","m","3","3","2.5","2.5","2.3","2.3","3","3","2.5","2.5","2.3","2.3","3","3","2.5","2.5","2.3","2.3","3","3","2.5","2.5","2.3","2.3"]
["Dimensions","Unité","Hauteur","mm","370","370","270","270","270","270","370","370","270","270","270","270","370","370","270","270","270","270","370","370","270","270","270","270"]
["","","Largeur","mm","1000","1000","1000","1000","1000","1000","1500","1500","1500","1500","1500","1500","2000","2000","2000","2000","2000","2000","2500","2500","2500","2500","2500","2500"]
["","","Profondeur","mm","774","774","590","590","590","590","774","774","590","590","590","590","774","774","590","590","590","590","774","774","590","590","590","590"]
["Poids","Unité","","kg","76","76","57","57","56","56","100","100","73","73","66","66","126","126","94","94","83","83","157","157","108","108","107","107"]
["Caisson","Couleur","","","RAL9016","RAL9006","RAL9016","RAL9006","RAL9016","RAL9006","RAL9016","RAL9006","RAL9016","RAL9006","RAL9016","RAL9006","RAL9016","RAL9006","RAL9016","RAL9006","RAL9016","RAL9006","RAL9016","RAL9006","RAL9016","RAL9006","RAL9016","RAL9006"]
["","Matériau","","","tôle d'acier électrozinguée","tôle d'acier électrozinguée","tôle d'acier électrozinguée","tôle d'acier électrozinguée","tôle d'acier électrozinguée","tôle d'acier électrozinguée","tôle d'acier électrozinguée","tôle d'acier électrozinguée","tôle d'acier électrozinguée","tôle d'acier électrozinguée","tôle d'acier électrozinguée","tôle d'acier électrozinguée","tôle d'acier électrozinguée","tôle d'acier électrozinguée","tôle d'acier électrozinguée","tôle d'acier électrozinguée","tôle d'acier électrozinguée","tôle d'acier électrozinguée","tôle d'acier électrozinguée","tôle d'acier électrozinguée","tôle d'acier électrozinguée","tôle d'acier électrozinguée","tôle d'acier électrozinguée","tôle d'acier électrozinguée"]
["Réfrigérant","Type","","","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A"]
["Raccords de tuyauterie","Liquide","DE","mm","9.52","9.52","6.35","6.35","6.35","6.35","9.52","9.52","6.35","6.35","6.35","6.35","9.52","9.52","9.52","9.52","9.52","9.52","9.52","9.52","9.52","9.52","9.52","9.52"]
["","Gaz","DE","mm","15.9","15.9","12.7","12.7","12.7","12.7","19.1","19.1","12.7","12.7","12.7","12.7","19.1","19.1","15.9","15.9","15.9","15.9","19.1","19.1","15.9","15.9","15.9","15.9"]
["Alimentation électrique","Alimentation électrique-=-Fréquence","Fréquence","","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50"]
["","Alimentation électrique-=-Tension","Alimentation électrique-=-Tension-=-V","","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230"]