{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":9,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVH-E6V / ERGA-EV7"]
[]
[]
[]
[]
["","","","","","EHVH04S18EA6V / ERGA04EAV37","EHVH04S18EJ6V / ERGA04EAV37","EHVH04S23EA6V / ERGA04EAV37","EHVH04S23EJ6V / ERGA04EAV37"]
["Puissance calorifique","Nom.","","","kW","4.36, 4.60","4.36, 4.60","4.36, 4.60","4.36, 4.60"]
["Puissance absorbée","Chauffage","","Nom.","kW","0.830, 1.26","0.830, 1.26","0.830, 1.26","0.830, 1.26"]
["","Eau chaude sanitaire de 10°C à 50°C","","Nom.","kWh","2.48","2.48","3.01","3.01"]
["Temps de montée en température de 10°C à 50°C-=-h","h","","","","1h28min","1h28min","1h40min","1h40min"]
["COP","","","","","5.23, 3.65","5.23, 3.65","5.23, 3.65","5.23, 3.65"]
["Chauffage d'eau chaude sanitaire","Général","","Profil de charge déclaré","","L","L","XL","XL"]
["","Climat moyen","","Classe","","A","A","A","A"]
["Chauffage des locaux","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 55 °C","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 55 °C-=-Général","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 55 °C-=-Général-=-SCOP","","3.26","3.26","3.26","3.26"]
["","","","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 55 °C-=-Général-=-Classe d'effic. saisonnière du chauffage d'ambiance","","A++","A++","A++","A++"]
["","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 35 °C","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 35 °C-=-Général","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 35 °C-=-Général-=-SCOP","","4.88","4.88","4.88","4.88"]
["","","","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 35 °C-=-Général-=-Classe d'effic. saisonnière du chauffage d'ambiance","","A+++","A+++","A+++","A+++"]
["Classe d'efficacité énergétique","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Remarques","","","","","(1) - Condition 1 : rafraîchissement Ta 35°C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1 : rafraîchissement Ta 35°C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1 : rafraîchissement Ta 35°C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1 : rafraîchissement Ta 35°C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition 2 : rafraîchissement Ta 35°C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7°C/6°C - LWC 45 °C (DT = 5°C)","(2) - Condition 2 : rafraîchissement Ta 35°C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7°C/6°C - LWC 45 °C (DT = 5°C)","(2) - Condition 2 : rafraîchissement Ta 35°C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7°C/6°C - LWC 45 °C (DT = 5°C)","(2) - Condition 2 : rafraîchissement Ta 35°C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7°C/6°C - LWC 45 °C (DT = 5°C)"]