{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":7,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHY2KOMB-A"]
[]
[]
[]
[]
["","","","","","EHY2KOMB28AA","EHY2KOMB32AA"]
["Eau chaude sanitaire","Apport de chaleur (valeur calorifique brute) Qnw","Nom.","Max.","kW","32.3","36.3"]
["","","","Min.","kW","7.9","8.4"]
["","Classe de confort (EN13203)","","","","XL","XL"]
["","Température","","Max.","°C","65","65"]
["","Apport de chaleur (valeur calorifique nette) Qnw","Nom.","Min.","kW","7.1","7.6"]
["","","","Max.","kW","29.1","32.7"]
["Gaz de carneau","Débit massique (G25)","","Max.","kg/h","48.6","54.4"]
["","Débit massique (G20)","","Max.","kg/h","48.6","54.4"]
["","Débit massique (G31)","","Max.","kg/h","47.9","53.6"]
["","Température","","Max.","°C","70","70"]
["Air d'alimentation","Concentrique","","","","60/100","60/100"]
["Production d'eau chaude sanitaire","Général","","Classe","","A","A"]
["","","","Profil de charge déclaré","","XL","XL"]
["Dimensions","Unité","Hauteur","Caisson","mm","650","710"]
["Caisson","Matériau","","","","Tôle avec précouche","Tôle avec précouche"]
["","Couleur","","","","RAL9010","RAL9010"]
["Chauffage des locaux","Général","","ηs (efficacité saisonnière du chauffage de l'air ambiant)","%","92","93"]
["","","","Classe d'efficacité saisonnière du chauffage de l'air ambiant","","A","A"]
["Chauff. central","Apport de chaleur Qn (valeur calorifique brute)","Nom.","Min.","kW","7.9","8.4"]
["","","","Max.","kW","26.3","30.0"]
["","Température de l'eau","","Max.","°C","90","90"]
["","Sortie à 37/30°C","","Nom.","kW","7.7","8.2"]
["","Sortie Pn à 80/60°C","","Min.","kW","7.1","7.4"]
["","","","Nom.","kW","23.1","26.6"]
["","Apport de chaleur Qn (valeur calorifique nette)","Nom.","Min.","kW","7.1","7.6"]
["","","","Max.","kW","23.7","27.0"]
["","Sortie Pnc à 50/30°C","","Min.","kW","7.7","8.2"]
["","","","Nom.","kW","25.4","28.9"]
["Gaz","Niveau NOx (G20)","","","mg/kWh","27","36"]
["","Consommation (G25)","","Min.","m³/h","0.84","0.89"]
["","","","Max.","m³/h","3.46","3.92"]
["","Catégorie NOx","","","","6","6"]
["","Connexion","","Diamètre","mm","15","15"]
["","Consommation (G20)","","Max.","m³/h","3.02","3.39"]
["","","","Min.","m³/h","0.74","0.79"]
["","Consommation (G31)","","Min.","m³/h","0.28","0.30"]
["","","","Max.","m³/h","1.15","1.29"]