{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKCB-CV3"]
[]
[]
[]
[]
["","","","","EKCB07CAV3"]
["Dimensions","Unité","Largeur","mm","340"]
["","","Profondeur","mm","97.0"]
["","","Hauteur","mm","360"]
["Caisson","Matériau","","","Tôle avec précouche"]
["","Couleur","","","Blanc"]
["Poids","Unité","","kg","4.00"]
["Raccords de câblage","Pour raccordement électrique au modèle *KHW* en option + Q2L","Remarque","","Section de câble 2,5 mm2"]
["","","Quantité","","4 + MASSE"]
["","Pour raccordement à l'interface utilisateur","Remarque","","100 mA, 0,75 mm² jusqu’à 1,25 mm² (longueur max. 500m)"]
["","","Quantité","","2"]
["Power supply","Phase","","","1~"]
["","Fréquence","","Hz","50"]
["","Tension","","V","230"]
["Courant","Fusibles recommandés","","A","10"]
["Remarques","","","","(1) - Équipement conforme à la norme EN/CEI 61000-3-12 : Norme technique internationale/européenne définissant les limites de courants harmoniques générés par les équipements connectés au système basse tension public avec un courant d'entrée > 16 A et ≤ 75 A par phase"]
["","","","","(2) - Entre *KCB*C* et *K2CB*C*"]
["","","","","(3) - Sélect. le diam. et le type selon les réglementations nationales et locales"]