{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":5,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKRTR"]
[]
[]
[]
[]
["","","","","EKRTR1"]
["Fonction de réglage","","","","Bande proportionnelle"]
["Dimensions","Récepteur","Hauteur","mm","170"]
["","","Profondeur","mm","28"]
["","","Largeur","mm","50"]
["","Thermostat","Profondeur","mm","34"]
["","","Largeur","mm","125"]
["","","Hauteur","mm","87"]
["Plage de réglage de température","Chauffage","Max.","°C","37"]
["","","Min.","°C","4"]
["","Rafraîchissement","Max.","°C","37"]
["","","Min.","°C","4"]
["Horloge","","","","Oui"]
["Poids","Récepteur","","g","125"]
["","Thermostat","","g","210"]
["Température extérieure","Stockage","Max.","°F","140"]
["","","Min.","°C","-20"]
["","","Max.","°C","60"]
["","","Min.","°F","-4"]
["","Fonctionnement","Min.","°C","0"]
["","","Max.","°F","122"]
["","","Min.","°F","32"]
["","","Max.","°C","50"]
["Courant de commutation nominal maximum (à 230 V CA)","A","","","4.0 (1)"]
["Distance maximum jusqu’au récepteur","Extérieur","","m","100 m environ"]
["","Intérieur","","m","30 m environ"]
["Connexion","Thermostat","","","Sans fil"]
["","Récepteur","","","Câblée"]
["Power supply","Phase","","","1~"]
["","Fréquence","","Hz","50"]
["","Récepteur","Tension","V","230"]
["","Thermostat","Tension","V","Alimentation par piles 3x AA-LRG (alcalines)"]
["Remarques","","","","(1) - 230 Vca"]