{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSK08-10AW1"]
[]
[]
[]
[]
["","","","","","EPSK08ARW1","EPSK10ARW1"]
["Dimensions","Unité","","Hauteur","mm","1123","1123"]
["","","","Largeur","mm","1330","1330"]
["","","","Profondeur","mm","604","604"]
["Poids","Unité","","","kg","178","178"]
["Ventilateur","Débit d'air","Chauffage","Haut","m³/min","75.7","75.7"]
["","","Rafraîchissement","Haut","m³/min","75.7","75.7"]
["Plage de fonct.","Rafraîch.","","Min.","°CBS","10","10"]
["","","","Max.","°CBS","43","43"]
["Plage de fonctionnement","Eau chaude domestique","","Min.","°CBS","-28","-28"]
["Plage de fonct.","Eau chaude sanitaire","","Max.","°CBS","40","40"]
["Niveau de puissance sonore","Chauffage","","Nom.","dBA","45 (1)","47 (1)"]
["","Rafraîchissement","","Nom.","dBA","53 (2)","53.2 (2)"]
["Niveau de pression sonore","Chauffage","","Nom.","dBA","32.4 (1)","32.8 (1)"]
["","Rafraîchissement","","Nom.","dBA","37.2 (2)","37.3 (2)"]
["Réfrigérant","","","","","R-290","R-290"]
["","Réfrigérant-=-PRP","","","","3","3"]
["","Réfrigérant-=-Charge-=-Téq. CO₂","","","Téq. CO₂","0.003","0.003"]
["","Charge","","","kg","1","1"]
["Raccords de tuyauterie","Dénivelé","UI - UE","Max.","m","10","10"]
["Alimentation électrique","Nom","","","","W1","W1"]
["","Phase","","","","3~","3~"]
["","Fréquence","","","Hz","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","400","400"]
["Courant","Fusibles recommandés","","","A","16","16"]
["Remarques","","","","","(1) - Mesuré à LWC 47-55°C ; Ta DB/WB 7°C/6°C.","(1) - Mesuré à LWC 47-55°C ; Ta DB/WB 7°C/6°C."]
["","","","","","(2) - Mesuré à LWC 12-7°C ; Ta 35°C.","(2) - Mesuré à LWC 12-7°C ; Ta 35°C."]
["","","","","","(3) - Tuyauterie sur le terrain 1 1/4\"","(3) - Tuyauterie sur le terrain 1 1/4\""]
["","","","","","(4) - Tuyauterie sur le terrain 1 1/2\"","(4) - Tuyauterie sur le terrain 1 1/2\""]