{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":11,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPVX10A4V / EPSK06-10AV3"]
[]
[]
[]
[]
["","","","","","EPVX10S18AJ4V / EPSK06ARV3","EPVX10S23AJ4V / EPSK06ARV3","EPVX10S18AJ4V / EPSK08ARV3","EPVX10S23AJ4V / EPSK08ARV3","EPVX10S18AJ4V / EPSK10ARV3","EPVX10S23AJ4V / EPSK10ARV3"]
["Unité intérieure","","","","","EPVX10S18AJ4V","EPVX10S23AJ4V","EPVX10S18AJ4V","EPVX10S23AJ4V","EPVX10S18AJ4V","EPVX10S23AJ4V"]
["Puissance calorifique","Nom.","","","kW","5.81 (1)","5.81 (1)","7.62 (1)","7.62 (1)","8.11 (1)","8.11 (1)"]
["Puissance frigorifique","Nom.","","","kW","6.00 (2), 6.37 (3)","6.00 (2), 6.37 (3)","6.89 (2), 6.37 (3)","6.89 (2), 6.37 (3)","7.84 (2), 6.37 (3)","7.84 (2), 6.37 (3)"]
["Puissance absorbée","Chauffage","","Nom.","kW","1.12 (1)","1.12 (1)","1.52 (1)","1.52 (1)","1.64 (1)","1.64 (1)"]
["","Rafraîchissement","","Nom.","kW","1.55 (2), 1.13 (3)","1.55 (2), 1.13 (3)","1.85 (2), 1.13 (3)","1.85 (2), 1.13 (3)","2.17 (2), 1.13 (3)","2.17 (2), 1.13 (3)"]
["","Eau chaude sanitaire de 10°C à 50°C","","Nom.","kWh","2.35","2.89","2.35","2.89","2.35","2.89"]
["Temps de montée en température de 10°C à 50°C-=-h","h","","","","1h 27min","1h 58min","1h 27min","1h 58min","1h 27min","1h 58min"]
["COP","","","","","5.19 (1)","5.19 (1)","5.01 (1)","5.01 (1)","4.94 (1)","4.94 (1)"]
["EER","","","","","3.87 (2), 5.63 (3)","3.87 (2), 5.63 (3)","3.73 (2), 5.63 (3)","3.73 (2), 5.63 (3)","3.62 (2), 5.63 (3)","3.62 (2), 5.63 (3)"]
["Chauffage d'eau chaude sanitaire","Général","","Profil de charge déclaré","","L","L","L","L","L","L"]
["","Climat moyen","","Classe","","A+","A+","A+","A+","A+","A+"]
["Chauffage des locaux","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 55 °C","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 55 °C-=-Général","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 55 °C-=-Général-=-SCOP","","3.91","3.91","3.97","3.97","4.02","4.02"]
["","","","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 55 °C-=-Général-=-Classe d'effic. saisonnière du chauffage d'ambiance","","A+++","A+++","A+++","A+++","A+++","A+++"]
["","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 35 °C","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 35 °C-=-Général","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 35 °C-=-Général-=-SCOP","","5.12","5.12","5.15","5.15","5.15","5.15"]
["","","","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 35 °C-=-Général-=-Classe d'effic. saisonnière du chauffage d'ambiance","","A+++","A+++","A+++","A+++","A+++","A+++"]
["Energy Efficiency Range","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Remarques","","","","","(1) - Condition : Ta DS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition : Ta DS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition : Ta DS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition : Ta DS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition : Ta DS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition : Ta DS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Rafraîchissement : Entrée d'eau 12°C ; Sortie d'eau 7°C ; Conditions extérieures : 35 °CBS","(2) - Rafraîchissement : Entrée d'eau 12°C ; Sortie d'eau 7°C ; Conditions extérieures : 35 °CBS","(2) - Rafraîchissement : Entrée d'eau 12°C ; Sortie d'eau 7°C ; Conditions extérieures : 35 °CBS","(2) - Rafraîchissement : Entrée d'eau 12°C ; Sortie d'eau 7°C ; Conditions extérieures : 35 °CBS","(2) - Rafraîchissement : Entrée d'eau 12°C ; Sortie d'eau 7°C ; Conditions extérieures : 35 °CBS","(2) - Rafraîchissement : Entrée d'eau 12°C ; Sortie d'eau 7°C ; Conditions extérieures : 35 °CBS"]
["","","","","","(3) - Rafraîchissement : Entrée d'eau 23°C ; Sortie d'eau 18°C ; Conditions extérieures : 35 °CBS","(3) - Rafraîchissement : Entrée d'eau 23°C ; Sortie d'eau 18°C ; Conditions extérieures : 35 °CBS","(3) - Rafraîchissement : Entrée d'eau 23°C ; Sortie d'eau 18°C ; Conditions extérieures : 35 °CBS","(3) - Rafraîchissement : Entrée d'eau 23°C ; Sortie d'eau 18°C ; Conditions extérieures : 35 °CBS","(3) - Rafraîchissement : Entrée d'eau 23°C ; Sortie d'eau 18°C ; Conditions extérieures : 35 °CBS","(3) - Rafraîchissement : Entrée d'eau 23°C ; Sortie d'eau 18°C ; Conditions extérieures : 35 °CBS"]