{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERGA-EV7"]
[]
[]
[]
[]
["","","","","","ERGA04EAV37"]
["Dimensions","Unité","","Hauteur","mm","740"]
["","","","Largeur","mm","884"]
["","","","Profondeur","mm","388"]
["Poids","Unité","","","kg","58.5"]
["Plage de fonct.","Rafraîch.","","Min.","°CBS","10"]
["","","","Max.","°CBS","43"]
["Plage de fonctionnement","Eau chaude domestique","","Min.","°CBS","-25"]
["Plage de fonct.","Eau chaude sanitaire","","Max.","°CBS","35"]
["Niveau de puissance sonore","Chauffage","","Nom.","dBA","58 (1)"]
["","Rafraîchissement","","Nom.","dBA","61 (1)"]
["Niveau de pression sonore","Chauffage","","Nom.","dBA","44 (1)"]
["","Rafraîchissement","","Nom.","dBA","48 (1)"]
["Réfrigérant","","","","","R-32"]
["","Réfrigérant-=-PRP","","","","675.0"]
["","Charge","","","tCO2Eq","1.01"]
["","Charge","","","kg","1.5"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35"]
["","Gaz","","DE","mm","15.9"]
["","Évacuation","","DE","mm","18"]
["","Dénivelé","UI - UE","Max.","m","20.0"]
["","Isolation thermique","","","","Tuyaux de liquide et tuyaux de gaz"]
["Alimentation électrique","Nom","","","","V3"]
["","Phase","","","","1N~"]
["","Fréquence","","","Hz","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","230"]
["Courant","Fusibles recommandés","","","A","20"]
["Remarques","","","","","(1) - Cooling Ta 35°C - LWE 18°C (DT = 5°C); Heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]