{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":60,"n_cols":8,"rows_kept":60,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERSQ-AV1"]
[]
[]
[]
[]
["","","","","","ERSQ011AAV1","ERSQ014AAV1","ERSQ016AAV1"]
["Niveau de pression sonore","Chauffage","","Nom.","dBA","","53"]
["Accessoires standard","Manuel d'installation","","","","","1"]
["Réfrigérant","PRP","","","","","2,087.5"]
["","Charge","","","kg","","4.5"]
["","Type","","","","","R-410A"]
["Plage de fonctionnement","Chauffage","","Max.","°CBH","","20"]
["","","","Min.","°CBH","","-20"]
["","Eau chaude domestique","","Min.","°CBS","","-20"]
["","","","Max.","°CBS","","35"]
["Raccords de tuyauterie","Isolation thermique","","","","","Tuyaux de liquide et tuyaux de gaz"]
["","Liquide","","DE","mm","","9.52"]
["","Gaz","","DE","mm","","15.9"]
["","Évacuation","","DE","mm","","26x3"]
["","Dénivelé","UI - UE","Max.","m","","30"]
["Sound power level","Heating","","Nom.","dBA","","69"]
["Dimensions","Unité","","Largeur","mm","","900"]
["","","","Profondeur","mm","","320"]
["","","","Hauteur","mm","","1,345"]
["Poids","Unité","","","kg","","120"]
["Power supply","Phase","","","","","1~"]
["","Nom","","","","","V1"]
["","Fréquence","","","Hz","","50"]
["","Tension","","","V","","220-440"]
["Courant","Fusibles recommandés","","","A","","25"]
["Remarques","","","","","","(1) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","","","(2) - Zmax : Conformément à la norme EN/CEI 61000-3-11, il peut s'avérer nécessaire de prendre contact avec l'opérateur du réseau de distribution d'électricité afin de s'assurer que l'équipement est connecté uniquement à une alimentation avec valeur Zsys (impédance système) ≤ Zmax."]
["","","","","","","(3) - EN/CEI 61000-3-11 : Norme technique européenne/internationale définissant les limites des variations de tension, des fluctuations de tension et des flickers sur les systèmes publics d'alimentation basse tension pour les équipements à intensités nominales <= 75 A"]
["","","","","","","(4) - Valeur Ssc (=puissance de court-circuit) minimum : Équipement conforme à la norme EN/CEI 61000-3-12 : Norme technique internationale/européenne définissant les limites de courants harmoniques générés par les équipements connectés aux systèmes basse tension publics avec un courant d'entrée > 16 A et ≤ 75 A par phase"]
["","","","","","","(5) - Contient des gaz à effet de serre fluorés."]
["Dimensions","Unité","","Hauteur","mm","1345","","1345"]
["","","","Largeur","mm","900","","900"]
["","","","Profondeur","mm","320","","320"]
["Poids","Unité","","","kg","120","","120"]
["Plage de fonctionnement","Chauffage","","Min.","°CBH","-20","","-20"]
["","","","Max.","°CBH","20","","20"]
["","Eau chaude domestique","","Min.","°CBS","-20","","-20"]
["Plage de fonct.","Eau chaude sanitaire","","Max.","°CBS","35","","35"]
["Niveau de puissance sonore","Chauffage","","Nom.","dBA","68","","71"]
["Niveau de pression sonore","Chauffage","","Nom.","dBA","52","","55"]
["Réfrigérant","","","","","R-410A","","R-410A"]
["","Réfrigérant-=-PRP","","","","2087.5","","2087.5"]
["","Charge","","","tCO2Eq","9.4","","9.4"]
["","Charge","","","kg","4.5","","4.5"]
["Raccords de tuyauterie","Liquide","","DE","mm","9.52","","9.52"]
["","Gaz","","DE","mm","15.9","","15.9"]
["","Évacuation","","DE","mm","26x3","","26x3"]
["","Dénivelé","UI - UE","Max.","m","30","","30"]
["","Isolation thermique","","","","Tuyaux de liquide et tuyaux de gaz","","Tuyaux de liquide et tuyaux de gaz"]
["Accessoires standard","Installation manual","","","","1","","1"]
["Alimentation électrique","Nom","","","","V1","","V1"]
["","Phase","","","","1~","","1~"]
["","Fréquence","","","Hz","50","","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-440","","220-440"]
["Courant","Fusibles recommandés","","","A","25","","25"]