{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C9 / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FAQ100CVEB9 / RZQG71L8Y1B","FAQ71CVEB9 / RZQG71L8Y1B","FAQ100CVEB9 / RZQG100L8Y1B","FAQ71CVEB9 / FAQ71CVEB9 / RZQG100L8Y1B","FAQ71CVEB9 / FAQ71CVEB9 / RZQG125L8Y1B"]
["Rafraîchissement de l'air ambiant","SEER","","","6.51","6.43","6.11","5.10","5.10"]
["","Consommation d’énergie annuelle","","kWh/a","366","371","545","652","824"]
["","Puissance","Pdesign","kW","6.80","6.80","9.50","9.50","12.00"]
["","Classe d’efficacité énergétique","","","A++","A++","A++","B","B"]
["Chauffage des locaux (climat tempéré)","Puissance","Pdesign","kW","6.33","6.33","10.20","11.30","12.71"]
["","SCOP/A","","","4.02","4.02","4.01","3.80","3.80"]
["","Classe d’efficacité énergétique","","","A+","A+","A+","A","A"]
["","Consommation d’énergie annuelle","","kWh/a","2,205","2,205","3,562","4,164","4,683"]
["Remarques","","","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]
["Puissance frigorifique","Nom.","","kW","","6.8","9.5"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","","1,000","1,315"]
["","EER","","","","3.40","3.62"]
["","COP","","","","3.70","3.61"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","","A","A"]
["","","Chauffage","","","A","A"]
["Puissance calorifique","Nom.","","kW","","7.5","10.8"]
["Remarques","","","","","(1) - La consommation énergétique annuelle est conforme à la directive 2002/31/CE sur l'étiquetage énergétique.","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]
["","","","","","(2) - Les valeurs SEER et SCOP sont conformes à la norme EN 14825.","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°"]