{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RXS-L"]
[]
[]
[]
[]
["","","","","FCAG50AVEB / RXS50L2V1B","FCAG60AVEB / RXS60L2V1B"]
["Puissance frigorifique","Nom.","","kW","5.00","5.70"]
["Rafraîchissement des locaux","SEER","","","6.48","6.22"]
["","Consommation d’énergie annuelle","","kWh/a","270","321"]
["","Puissance","Pdesign","kW","5.00","5.70"]
["","Classe d’efficacité énergétique","","","A++","A++"]
["Chauffage des locaux (climat tempéré)","Puissance","Pdesign","kW","4.36","4.71"]
["","SCOP/A","","","4.29","4.00"]
["","Classe d’efficacité énergétique","","","A++","A+"]
["","Consommation d’énergie annuelle","","kWh/a","1,426","1,646"]
["Raccords de tuyauterie","Liquide","DE","mm","6.35","6.35"]
["","Gaz","DE","mm","12.70","12.70"]
["","Évacuation","DE","mm","VP25 (diamètre ext. : 32 / diamètre int. : 25)","VP25 (diamètre ext. : 32 / diamètre int. : 25)"]
["Efficacité nominale","EER","","","3.55","3.48"]
["","Consommation énergétique annuelle","","kWh","705","820"]
["","COP","","","3.70","3.52"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","A"]
["","","Chauffage","","A","B"]
["Puissance calorifique","Nom.","","kW","6.00","7.00"]
["Remarques","","","","(1) - Les puissances frigorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m.","(1) - Les puissances frigorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m."]
["","","","","(2) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m.","(2) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m."]
["","","","","(3) - Voir le schéma séparé pour la plage de fonctionnement","(3) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","(4) - Pour les données électriques, se reporter au schéma séparé.","(4) - Pour les données électriques, se reporter au schéma séparé."]